(footprint "SSOP-8_2.95x2.8mm_P0.65mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "SSOP-8 2.9 x2.8mm Pitch 0.65mm")
	(tags "SSOP-8 2.95x2.8mm Pitch 0.65mm")
	(property "Reference" "REF**"
		(at 0 -2.4 0)
		(layer "F.SilkS")
	)
	(property "Value" "SSOP-8_2.95x2.8mm_P0.65mm"
		(at 0 2.6 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -1.7 -0.975 270)
		(size 0.3 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -1.7 -0.325 270)
		(size 0.3 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -1.7 0.325 270)
		(size 0.3 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -1.7 0.975 270)
		(size 0.3 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at 1.7 0.975 270)
		(size 0.3 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at 1.7 0.325 270)
		(size 0.3 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at 1.7 -0.325 270)
		(size 0.3 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at 1.7 -0.975 270)
		(size 0.3 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_SO.3dshapes/SSOP-8_2.95x2.8mm_P0.65mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
