(footprint "SSOP-8_5.25x5.24mm_P1.27mm"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "SSOP, 8 Pin (http://www.fujitsu.com/ca/en/Images/MB85RS2MT-DS501-00023-1v0-E.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
	(tags "SSOP SO")
	(property "Reference" "REF**"
		(at 0 -3.57 0)
		(layer "F.SilkS")
	)
	(property "Value" "SSOP-8_5.25x5.24mm_P1.27mm"
		(at 0 3.57 0)
		(layer "F.Fab")
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -3.6125 -1.905)
		(size 1.725 0.6)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -3.6125 -0.635)
		(size 1.725 0.6)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at -3.6125 0.635)
		(size 1.725 0.6)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at -3.6125 1.905)
		(size 1.725 0.6)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at 3.6125 1.905)
		(size 1.725 0.6)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "6" smd roundrect
		(at 3.6125 0.635)
		(size 1.725 0.6)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "7" smd roundrect
		(at 3.6125 -0.635)
		(size 1.725 0.6)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "8" smd roundrect
		(at 3.6125 -1.905)
		(size 1.725 0.6)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(model "${KICAD9_3DMODEL_DIR}/Package_SO.3dshapes/SSOP-8_5.25x5.24mm_P1.27mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
