(footprint "TSOP-I-28_11.8x8mm_P0.55mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "TSOP I, 28 pins, 18.8x8mm body, 0.55mm pitch, IPC-calculated pads (http://ww1.microchip.com/downloads/en/devicedoc/doc0807.pdf)")
	(tags "TSOP I 28 pins")
	(property "Reference" "REF**"
		(at 0.5 -5.1 0)
		(layer "F.SilkS")
	)
	(property "Value" "TSOP-I-28_11.8x8mm_P0.55mm"
		(at 0 5.7 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0.5 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -6.27 -3.575)
		(size 1.87 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -6.27 -3.025)
		(size 1.87 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -6.27 -2.475)
		(size 1.87 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -6.27 -1.925)
		(size 1.87 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -6.27 -1.375)
		(size 1.87 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at -6.27 -0.825)
		(size 1.87 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at -6.27 -0.275)
		(size 1.87 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at -6.27 0.275)
		(size 1.87 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at -6.27 0.825)
		(size 1.87 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at -6.27 1.375)
		(size 1.87 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at -6.27 1.925)
		(size 1.87 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd rect
		(at -6.27 2.475)
		(size 1.87 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd rect
		(at -6.27 3.025)
		(size 1.87 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd rect
		(at -6.27 3.575)
		(size 1.87 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "15" smd rect
		(at 6.27 3.575)
		(size 1.87 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "16" smd rect
		(at 6.27 3.025)
		(size 1.87 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "17" smd rect
		(at 6.27 2.475)
		(size 1.87 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "18" smd rect
		(at 6.27 1.925)
		(size 1.87 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "19" smd rect
		(at 6.27 1.375)
		(size 1.87 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "20" smd rect
		(at 6.27 0.825)
		(size 1.87 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "21" smd rect
		(at 6.27 0.275)
		(size 1.87 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "22" smd rect
		(at 6.27 -0.275)
		(size 1.87 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "23" smd rect
		(at 6.27 -0.825)
		(size 1.87 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "24" smd rect
		(at 6.27 -1.375)
		(size 1.87 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "25" smd rect
		(at 6.27 -1.925)
		(size 1.87 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "26" smd rect
		(at 6.27 -2.475)
		(size 1.87 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "27" smd rect
		(at 6.27 -3.025)
		(size 1.87 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "28" smd rect
		(at 6.27 -3.575)
		(size 1.87 0.38)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_SO.3dshapes/TSOP-I-28_11.8x8mm_P0.55mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
