(footprint "TSOP-I-32_18.4x8mm_P0.5mm_Reverse"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "TSOP I, 32 pins, 18.4x8mm body (http://www.futurlec.com/Datasheet/Memory/628128.pdf), reverse mount")
	(tags "TSOP I 32 reverse")
	(property "Reference" "REF**"
		(at 0 -11.3 0)
		(layer "F.SilkS")
	)
	(property "Value" "TSOP-I-32_18.4x8mm_P0.5mm_Reverse"
		(at 0 11.3 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -3.75 -9.75)
		(size 0.25 1.1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -3.25 -9.75)
		(size 0.25 1.1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -2.75 -9.75)
		(size 0.25 1.1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -2.25 -9.75)
		(size 0.25 1.1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -1.75 -9.75)
		(size 0.25 1.1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at -1.25 -9.75)
		(size 0.25 1.1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at -0.75 -9.75)
		(size 0.25 1.1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at -0.25 -9.75)
		(size 0.25 1.1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at 0.25 -9.75)
		(size 0.25 1.1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at 0.75 -9.75)
		(size 0.25 1.1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at 1.25 -9.75)
		(size 0.25 1.1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd rect
		(at 1.75 -9.75)
		(size 0.25 1.1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd rect
		(at 2.25 -9.75)
		(size 0.25 1.1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd rect
		(at 2.75 -9.75)
		(size 0.25 1.1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "15" smd rect
		(at 3.25 -9.75)
		(size 0.25 1.1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "16" smd rect
		(at 3.75 -9.75)
		(size 0.25 1.1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "17" smd rect
		(at 3.75 9.75)
		(size 0.25 1.1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "18" smd rect
		(at 3.25 9.75)
		(size 0.25 1.1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "19" smd rect
		(at 2.75 9.75)
		(size 0.25 1.1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "20" smd rect
		(at 2.25 9.75)
		(size 0.25 1.1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "21" smd rect
		(at 1.75 9.75)
		(size 0.25 1.1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "22" smd rect
		(at 1.25 9.75)
		(size 0.25 1.1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "23" smd rect
		(at 0.75 9.75)
		(size 0.25 1.1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "24" smd rect
		(at 0.25 9.75)
		(size 0.25 1.1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "25" smd rect
		(at -0.25 9.75)
		(size 0.25 1.1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "26" smd rect
		(at -0.75 9.75)
		(size 0.25 1.1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "27" smd rect
		(at -1.25 9.75)
		(size 0.25 1.1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "28" smd rect
		(at -1.75 9.75)
		(size 0.25 1.1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "29" smd rect
		(at -2.25 9.75)
		(size 0.25 1.1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "30" smd rect
		(at -2.75 9.75)
		(size 0.25 1.1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "31" smd rect
		(at -3.25 9.75)
		(size 0.25 1.1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "32" smd rect
		(at -3.75 9.75)
		(size 0.25 1.1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_SO.3dshapes/TSOP-I-32_18.4x8mm_P0.5mm_Reverse.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
