(footprint "TSSOP-14-1EP_4.4x5mm_P0.65mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "14-Lead Plastic Thin Shrink Small Outline (ST)-4.4 mm Body [TSSOP] with exposed pad (http://cds.linear.com/docs/en/datasheet/34301fa.pdf)")
	(tags "SSOP 0.65 exposed pad")
	(property "Reference" "REF**"
		(at 0 -3.55 0)
		(layer "F.SilkS")
	)
	(property "Value" "TSSOP-14-1EP_4.4x5mm_P0.65mm"
		(at 0 3.55 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -2.95 -1.95)
		(size 1.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -2.95 -1.3)
		(size 1.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -2.95 -0.65)
		(size 1.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -2.95 0)
		(size 1.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -2.95 0.65)
		(size 1.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at -2.95 1.3)
		(size 1.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at -2.95 1.95)
		(size 1.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at 2.95 1.95)
		(size 1.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at 2.95 1.3)
		(size 1.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at 2.95 0.65)
		(size 1.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at 2.95 0)
		(size 1.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd rect
		(at 2.95 -0.65)
		(size 1.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd rect
		(at 2.95 -1.3)
		(size 1.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd rect
		(at 2.95 -1.95)
		(size 1.45 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "15" smd rect
		(at -0.75 -0.9)
		(size 1.5 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.2)
	)
	(pad "15" smd rect
		(at -0.75 0.9)
		(size 1.5 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.2)
	)
	(pad "15" smd rect
		(at 0.75 -0.9)
		(size 1.5 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.2)
	)
	(pad "15" smd rect
		(at 0.75 0.9)
		(size 1.5 1.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.2)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_SO.3dshapes/TSSOP-14-1EP_4.4x5mm_P0.65mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
