(footprint "TSSOP-16-1EP_4.4x5mm_P0.65mm_EP3x3mm_ThermalVias"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "TSSOP, 16 Pin (Allegro A4954 https://www.allegromicro.com/-/media/Files/Datasheets/A4954-Datasheet.ashx), generated with kicad-footprint-generator ipc_gullwing_generator.py")
	(tags "TSSOP SO")
	(property "Reference" "REF**"
		(at 0 -3.45 0)
		(layer "F.SilkS")
	)
	(property "Value" "TSSOP-16-1EP_4.4x5mm_P0.65mm_EP3x3mm_ThermalVias"
		(at 0 3.45 0)
		(layer "F.Fab")
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd roundrect
		(at -0.75 -0.75)
		(size 1.21 1.21)
		(layers "F.Paste")
		(roundrect_rratio 0.206612)
	)
	(pad "" smd roundrect
		(at -0.75 0.75)
		(size 1.21 1.21)
		(layers "F.Paste")
		(roundrect_rratio 0.206612)
	)
	(pad "" smd roundrect
		(at 0.75 -0.75)
		(size 1.21 1.21)
		(layers "F.Paste")
		(roundrect_rratio 0.206612)
	)
	(pad "" smd roundrect
		(at 0.75 0.75)
		(size 1.21 1.21)
		(layers "F.Paste")
		(roundrect_rratio 0.206612)
	)
	(pad "1" smd roundrect
		(at -2.875 -2.275)
		(size 1.55 0.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -2.875 -1.625)
		(size 1.55 0.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at -2.875 -0.975)
		(size 1.55 0.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at -2.875 -0.325)
		(size 1.55 0.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at -2.875 0.325)
		(size 1.55 0.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "6" smd roundrect
		(at -2.875 0.975)
		(size 1.55 0.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "7" smd roundrect
		(at -2.875 1.625)
		(size 1.55 0.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "8" smd roundrect
		(at -2.875 2.275)
		(size 1.55 0.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "9" smd roundrect
		(at 2.875 2.275)
		(size 1.55 0.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "10" smd roundrect
		(at 2.875 1.625)
		(size 1.55 0.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "11" smd roundrect
		(at 2.875 0.975)
		(size 1.55 0.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "12" smd roundrect
		(at 2.875 0.325)
		(size 1.55 0.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "13" smd roundrect
		(at 2.875 -0.325)
		(size 1.55 0.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "14" smd roundrect
		(at 2.875 -0.975)
		(size 1.55 0.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "15" smd roundrect
		(at 2.875 -1.625)
		(size 1.55 0.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "16" smd roundrect
		(at 2.875 -2.275)
		(size 1.55 0.4)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "17" thru_hole circle
		(at -1.2 -1.2)
		(size 0.6 0.6)
		(drill 0.3)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "17" thru_hole circle
		(at -1.2 1.2)
		(size 0.6 0.6)
		(drill 0.3)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "17" smd rect
		(at 0 0)
		(size 3 3)
		(property pad_prop_heatsink)
		(layers "F.Cu" "F.Mask")
		(zone_connect 2)
	)
	(pad "17" smd rect
		(at 0 0)
		(size 3 3)
		(property pad_prop_heatsink)
		(layers "B.Cu")
		(zone_connect 2)
	)
	(pad "17" thru_hole circle
		(at 1.2 -1.2)
		(size 0.6 0.6)
		(drill 0.3)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "17" thru_hole circle
		(at 1.2 1.2)
		(size 0.6 0.6)
		(drill 0.3)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(model "${KICAD9_3DMODEL_DIR}/Package_SO.3dshapes/TSSOP-16-1EP_4.4x5mm_P0.65mm_EP3x3mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
