(footprint "Texas_DGN0008G_VSSOP-8-1EP_3x3mm_P0.65mm_EP2x2.94mm_Mask1.846x2.15mm_ThermalVias"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "Texas DGN0008G VSSOP, 8 Pin (https://www.ti.com/lit/ds/symlink/tpa711.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
	(tags "Texas VSSOP SO")
	(property "Reference" "REF**"
		(at 0 -2.45 0)
		(layer "F.SilkS")
	)
	(property "Value" "Texas_DGN0008G_VSSOP-8-1EP_3x3mm_P0.65mm_EP2x2.94mm_Mask1.846x2.15mm_ThermalVias"
		(at 0 2.45 0)
		(layer "F.Fab")
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd custom
		(at -0.7365 -0.5375)
		(size 0.191615 0.191615)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.092923 -0.396897)
					(xy 0.092923 -0.396897)
					(xy 0.092923 0.251232)
					(xy -0.052743 0.396897)
					(xy -0.092923 0.396897)
				)
				(width 0.137182)
			)
		)
	)
	(pad "" smd custom
		(at -0.7365 0.5375)
		(size 0.191615 0.191615)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.092923 -0.396897)
					(xy -0.052743 -0.396897)
					(xy 0.092923 -0.251232)
					(xy 0.092923 0.396897)
					(xy -0.092923 0.396897)
				)
				(width 0.137182)
			)
		)
	)
	(pad "" smd custom
		(at 0 -0.5375)
		(size 0.834001 0.834001)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.379338 -0.368512)
					(xy 0.379338 -0.368512)
					(xy 0.379338 0.288174)
					(xy 0.299 0.368512)
					(xy -0.299 0.368512)
					(xy -0.379338 0.288174)
				)
				(width 0.193953)
			)
		)
	)
	(pad "" smd rect
		(at 0 0)
		(size 1.846 2.15)
		(layers "F.Mask")
	)
	(pad "" smd custom
		(at 0 0.5375)
		(size 0.834001 0.834001)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.379338 -0.288174)
					(xy -0.299 -0.368512)
					(xy 0.299 -0.368512)
					(xy 0.379338 -0.288174)
					(xy 0.379338 0.368512)
					(xy -0.379338 0.368512)
				)
				(width 0.193953)
			)
		)
	)
	(pad "" smd custom
		(at 0.7365 -0.5375)
		(size 0.191615 0.191615)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.092923 -0.396897)
					(xy 0.092923 -0.396897)
					(xy 0.092923 0.396897)
					(xy 0.052743 0.396897)
					(xy -0.092923 0.251232)
				)
				(width 0.137182)
			)
		)
	)
	(pad "" smd custom
		(at 0.7365 0.5375)
		(size 0.191615 0.191615)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.092923 -0.251232)
					(xy 0.052743 -0.396897)
					(xy 0.092923 -0.396897)
					(xy 0.092923 0.396897)
					(xy -0.092923 0.396897)
				)
				(width 0.137182)
			)
		)
	)
	(pad "1" smd roundrect
		(at -2.2 -0.975)
		(size 1.45 0.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -2.2 -0.325)
		(size 1.45 0.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at -2.2 0.325)
		(size 1.45 0.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at -2.2 0.975)
		(size 1.45 0.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at 2.2 0.975)
		(size 1.45 0.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "6" smd roundrect
		(at 2.2 0.325)
		(size 1.45 0.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "7" smd roundrect
		(at 2.2 -0.325)
		(size 1.45 0.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "8" smd roundrect
		(at 2.2 -0.975)
		(size 1.45 0.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "9" thru_hole circle
		(at -0.55 -1.22)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "9" thru_hole circle
		(at -0.55 0)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "9" thru_hole circle
		(at -0.55 1.22)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "9" smd rect
		(at 0 0)
		(size 1.6 2.94)
		(property pad_prop_heatsink)
		(layers "B.Cu")
		(zone_connect 2)
	)
	(pad "9" smd rect
		(at 0 0)
		(size 2 2.94)
		(property pad_prop_heatsink)
		(layers "F.Cu")
		(zone_connect 2)
	)
	(pad "9" thru_hole circle
		(at 0.55 -1.22)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "9" thru_hole circle
		(at 0.55 0)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "9" thru_hole circle
		(at 0.55 1.22)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(model "${KICAD9_3DMODEL_DIR}/Package_SO.3dshapes/Texas_DGN0008G_VSSOP-8-1EP_3x3mm_P0.65mm_EP2x2.94mm_Mask1.846x2.15mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
