(footprint "Texas_PWP0020A"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "20-Pin Thermally Enhanced Thin Shrink Small-Outline Package, Body 4.4x6.5x1.1mm, Pad 3.0x4.2mm, Texas Instruments (see http://www.ti.com/lit/ds/symlink/lm5118.pdf)")
	(tags "PWP HTSSOP 0.65mm")
	(property "Reference" "REF**"
		(at 0 -4.5 0)
		(layer "F.SilkS")
	)
	(property "Value" "Texas_PWP0020A"
		(at 0 4.5 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(clearance 0.2)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd rect
		(at -0.7125 -1.0125)
		(size 1.275 1.875)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -0.7125 1.0125)
		(size 1.275 1.875)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.7125 -1.0125)
		(size 1.275 1.875)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.7125 1.0125)
		(size 1.275 1.875)
		(layers "F.Paste")
	)
	(pad "1" smd rect
		(at -2.97 -2.925)
		(size 1.78 0.42)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -2.97 -2.275)
		(size 1.78 0.42)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -2.97 -1.625)
		(size 1.78 0.42)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -2.97 -0.975)
		(size 1.78 0.42)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -2.97 -0.325)
		(size 1.78 0.42)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at -2.97 0.325)
		(size 1.78 0.42)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at -2.97 0.975)
		(size 1.78 0.42)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at -2.97 1.625)
		(size 1.78 0.42)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at -2.97 2.275)
		(size 1.78 0.42)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at -2.97 2.925)
		(size 1.78 0.42)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at 2.97 2.925)
		(size 1.78 0.42)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd rect
		(at 2.97 2.275)
		(size 1.78 0.42)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd rect
		(at 2.97 1.625)
		(size 1.78 0.42)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd rect
		(at 2.97 0.975)
		(size 1.78 0.42)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "15" smd rect
		(at 2.97 0.325)
		(size 1.78 0.42)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "16" smd rect
		(at 2.97 -0.325)
		(size 1.78 0.42)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "17" smd rect
		(at 2.97 -0.975)
		(size 1.78 0.42)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "18" smd rect
		(at 2.97 -1.625)
		(size 1.78 0.42)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "19" smd rect
		(at 2.97 -2.275)
		(size 1.78 0.42)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "20" smd rect
		(at 2.97 -2.925)
		(size 1.78 0.42)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "21" smd rect
		(at 0 0)
		(size 3 4.2)
		(layers "F.Cu" "F.Mask")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_SO.3dshapes/Texas_PWP0020A.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
