(footprint "VSO-40_7.6x15.4mm_P0.762mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "VSO40: plastic very small outline package; 40 leads (see NXP SSOP-TSSOP-VSO-REFLOW.pdf and sot158-1_po.pdf)")
	(tags "SSOP 0.762")
	(property "Reference" "REF**"
		(at 0 -8.8 0)
		(layer "F.SilkS")
	)
	(property "Value" "VSO-40_7.6x15.4mm_P0.762mm"
		(at 0 8.8 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -5.2 -7.239)
		(size 2.2 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -5.2 -6.477)
		(size 2.2 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -5.2 -5.715)
		(size 2.2 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -5.2 -4.953)
		(size 2.2 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -5.2 -4.191)
		(size 2.2 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at -5.2 -3.429)
		(size 2.2 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at -5.2 -2.667)
		(size 2.2 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at -5.2 -1.905)
		(size 2.2 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at -5.2 -1.143)
		(size 2.2 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at -5.2 -0.381)
		(size 2.2 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at -5.2 0.381)
		(size 2.2 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd rect
		(at -5.2 1.143)
		(size 2.2 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd rect
		(at -5.2 1.905)
		(size 2.2 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd rect
		(at -5.2 2.667)
		(size 2.2 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "15" smd rect
		(at -5.2 3.429)
		(size 2.2 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "16" smd rect
		(at -5.2 4.191)
		(size 2.2 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "17" smd rect
		(at -5.2 4.953)
		(size 2.2 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "18" smd rect
		(at -5.2 5.715)
		(size 2.2 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "19" smd rect
		(at -5.2 6.477)
		(size 2.2 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "20" smd rect
		(at -5.2 7.239)
		(size 2.2 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "21" smd rect
		(at 5.2 7.239)
		(size 2.2 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "22" smd rect
		(at 5.2 6.477)
		(size 2.2 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "23" smd rect
		(at 5.2 5.715)
		(size 2.2 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "24" smd rect
		(at 5.2 4.953)
		(size 2.2 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "25" smd rect
		(at 5.2 4.191)
		(size 2.2 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "26" smd rect
		(at 5.2 3.429)
		(size 2.2 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "27" smd rect
		(at 5.2 2.667)
		(size 2.2 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "28" smd rect
		(at 5.2 1.905)
		(size 2.2 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "29" smd rect
		(at 5.2 1.143)
		(size 2.2 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "30" smd rect
		(at 5.2 0.381)
		(size 2.2 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "31" smd rect
		(at 5.2 -0.381)
		(size 2.2 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "32" smd rect
		(at 5.2 -1.143)
		(size 2.2 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "33" smd rect
		(at 5.2 -1.905)
		(size 2.2 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "34" smd rect
		(at 5.2 -2.667)
		(size 2.2 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "35" smd rect
		(at 5.2 -3.429)
		(size 2.2 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "36" smd rect
		(at 5.2 -4.191)
		(size 2.2 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "37" smd rect
		(at 5.2 -4.953)
		(size 2.2 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "38" smd rect
		(at 5.2 -5.715)
		(size 2.2 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "39" smd rect
		(at 5.2 -6.477)
		(size 2.2 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "40" smd rect
		(at 5.2 -7.239)
		(size 2.2 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_SO.3dshapes/VSO-40_7.6x15.4mm_P0.762mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
