(footprint "Vishay_PowerPAK_1212-8_Single"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "PowerPAK 1212-8 Single (https://www.vishay.com/docs/71656/ppak12128.pdf, https://www.vishay.com/docs/72597/72597.pdf)")
	(tags "Vishay PowerPAK 1212-8 Single")
	(property "Reference" "REF**"
		(at 0 -2.7 0)
		(layer "F.SilkS")
	)
	(property "Value" "Vishay_PowerPAK_1212-8_Single"
		(at 0 2.7 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -1.435 -0.99)
		(size 0.99 0.405)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -1.435 -0.33)
		(size 0.99 0.405)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -1.435 0.33)
		(size 0.99 0.405)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -1.435 0.99)
		(size 0.99 0.405)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd custom
		(at 0.5575 0)
		(size 1.725 2.235)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy 1.3725 -0.7875) (xy 0.8625 -0.7875) (xy 0.8625 -0.5325) (xy 1.3725 -0.5325) (xy 1.3725 -0.1275)
					(xy 0.8625 -0.1275) (xy 0.8625 0.1275) (xy 1.3725 0.1275) (xy 1.3725 0.5325) (xy 0.8625 0.5325)
					(xy 0.8625 0.7875) (xy 1.3725 0.7875) (xy 1.3725 1.195) (xy 0.6125 1.195) (xy 0.6125 -1.195) (xy 1.3725 -1.195)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_SO.3dshapes/Vishay_PowerPAK_1212-8_Single.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
