(footprint "Diodes_PowerDI3333-8"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Diodes Incorporated PowerDI3333-8, Plastic Dual Flat No Lead Package, 3.3x3.3x0.8mm Body, https://www.diodes.com/assets/Package-Files/PowerDI3333-8.pdf")
	(tags "PowerDI 0.65")
	(property "Reference" "REF**"
		(at 0 -2.65 0)
		(layer "F.SilkS")
	)
	(property "Value" "Diodes_PowerDI3333-8"
		(at 0 2.65 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd roundrect
		(at 0.02 -0.565)
		(size 0.6 1)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(solder_paste_margin_ratio -0.2)
	)
	(pad "" smd roundrect
		(at 0.02 0.565)
		(size 0.6 1)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(solder_paste_margin_ratio -0.2)
	)
	(pad "" smd roundrect
		(at 0.73 -0.565)
		(size 0.6 1)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(solder_paste_margin_ratio -0.2)
	)
	(pad "" smd roundrect
		(at 0.73 0.565)
		(size 0.6 1)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(solder_paste_margin_ratio -0.2)
	)
	(pad "" smd roundrect
		(at 1.5 -0.975)
		(size 0.7 0.42)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 1.5 -0.325)
		(size 0.7 0.42)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 1.5 0.325)
		(size 0.7 0.42)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 1.5 0.975)
		(size 0.7 0.42)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "1" smd roundrect
		(at -1.5 -0.975)
		(size 0.7 0.42)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -1.5 -0.325)
		(size 0.7 0.42)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at -1.5 0.325)
		(size 0.7 0.42)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at -1.5 0.975)
		(size 0.7 0.42)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd custom
		(at 0.455 0)
		(size 1.71 2.37)
		(layers "F.Cu" "F.Mask")
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy 1.395 1.185) (xy 0.855 1.185) (xy 0.855 0.765) (xy 1.395 0.765)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 1.395 0.535) (xy 0.855 0.535) (xy 0.855 0.115) (xy 1.395 0.115)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 1.395 -0.115) (xy 0.855 -0.115) (xy 0.855 -0.535) (xy 1.395 -0.535)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 1.395 -0.765) (xy 0.855 -0.765) (xy 0.855 -1.185) (xy 1.395 -1.185)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_SON.3dshapes/Diodes_PowerDI3333-8.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
