(footprint "Diodes_PowerDI3333-8_UXC_3.3x3.3mm_P0.65mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Diodes Incorporated PowerDI3333-8 UXC, 3.05x3.05x0.8mm Body, https://www.diodes.com/assets/Package-Files/PowerDI3333-8%20(Type%20UXC).pdf")
	(tags "PowerDI 0.65")
	(property "Reference" "REF**"
		(at 0 -2.4 0)
		(layer "F.SilkS")
	)
	(property "Value" "Diodes_PowerDI3333-8_UXC_3.3x3.3mm_P0.65mm"
		(at 0 3.4 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 180)
		(layer "F.Fab")
	)
	(pad "" smd roundrect
		(at -0.22 -0.73)
		(size 0.6 1)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(solder_paste_margin_ratio -0.2)
	)
	(pad "" smd roundrect
		(at -0.22 0.71)
		(size 0.6 1)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(solder_paste_margin_ratio -0.2)
	)
	(pad "" smd roundrect
		(at 0.6 -0.73)
		(size 0.6 1)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(solder_paste_margin_ratio -0.2)
	)
	(pad "" smd roundrect
		(at 0.6 0.71)
		(size 0.6 1)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(solder_paste_margin_ratio -0.2)
	)
	(pad "" smd roundrect
		(at 1.45 -0.98)
		(size 0.7 0.4)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 1.45 -0.32)
		(size 0.7 0.4)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 1.45 0.32)
		(size 0.7 0.4)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 1.45 0.98)
		(size 0.7 0.4)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "1" smd roundrect
		(at -1.5 -0.975 270)
		(size 0.42 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "2" smd roundrect
		(at -1.5 -0.325 270)
		(size 0.42 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "3" smd roundrect
		(at -1.5 0.325 270)
		(size 0.42 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "4" smd roundrect
		(at -1.5 0.975 270)
		(size 0.42 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "5" smd custom
		(at 0.35 0.715 270)
		(size 1 1)
		(layers "F.Cu" "F.Mask")
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.6 0.95) (xy 0.6 0.95) (xy 0.6 -0.95) (xy 0.47 -0.95) (xy 0.47 -1.45) (xy 0.05 -1.45) (xy 0.05 -0.95)
					(xy -0.18 -0.95) (xy -0.18 -1.45) (xy -0.6 -1.45)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "7" smd custom
		(at 0.35 -0.715 270)
		(size 1 1)
		(layers "F.Cu" "F.Mask")
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.6 0.95) (xy -0.6 0.95) (xy -0.6 -0.95) (xy -0.47 -0.95) (xy -0.47 -1.45) (xy -0.05 -1.45)
					(xy -0.05 -0.95) (xy 0.18 -0.95) (xy 0.18 -1.45) (xy 0.6 -1.45)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_SON.3dshapes/Diodes_PowerDI3333-8_UXC_3.3x3.3mm_P0.65mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
