(footprint "Fairchild_DualPower33-6_3x3mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Fairchild Power33 MOSFET package, 3x3mm (see https://www.fairchildsemi.com/datasheets/FD/FDMC8032L.pdf)")
	(tags "mosfet")
	(property "Reference" "REF**"
		(at 0 -2.5 0)
		(layer "F.SilkS")
	)
	(property "Value" "Fairchild_DualPower33-6_3x3mm"
		(at 0 2.4 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd roundrect
		(at -1.39 -0.975)
		(size 0.35 0.35)
		(layers "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -1.39 -0.325)
		(size 0.35 0.35)
		(layers "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -1.39 0.325)
		(size 0.35 0.35)
		(layers "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -1.39 0.975)
		(size 0.35 0.35)
		(layers "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -0.55 -0.5)
		(size 0.65 0.8)
		(layers "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -0.55 0.5)
		(size 0.65 0.8)
		(layers "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 0.55 -0.5)
		(size 0.65 0.8)
		(layers "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 0.55 0.5)
		(size 0.65 0.8)
		(layers "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 1.39 -0.975)
		(size 0.35 0.35)
		(layers "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 1.39 -0.325)
		(size 0.35 0.35)
		(layers "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 1.39 0.325)
		(size 0.35 0.35)
		(layers "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 1.39 0.975)
		(size 0.35 0.35)
		(layers "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "1" smd roundrect
		(at -1.39 -0.975)
		(size 0.52 0.45)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -1.39 0.325)
		(size 0.52 1.75)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at 1.39 0.325)
		(size 0.52 1.75)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at 1.39 -0.975)
		(size 0.52 0.45)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at -0.55 0)
		(size 0.75 2.52)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "6" smd roundrect
		(at 0.55 0)
		(size 0.75 2.52)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_SON.3dshapes/Fairchild_DualPower33-6_3x3mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
