(footprint "Fairchild_MicroPak-6_1.0x1.45mm_P0.5mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Fairchild-specific MicroPak-6 1.0x1.45mm Pitch 0.5mm https://www.nxp.com/docs/en/application-note/AN10343.pdff")
	(tags "Fairchild-specific MicroPak-6 1.0x1.45mm Pitch 0.5mm")
	(property "Reference" "REF**"
		(at 0 -1.98 0)
		(layer "F.SilkS")
	)
	(property "Value" "Fairchild_MicroPak-6_1.0x1.45mm_P0.5mm"
		(at 0.0325 1.75 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0.0075 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -0.3675 -0.5)
		(size 0.52 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -0.3675 0)
		(size 0.52 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at -0.3675 0.5)
		(size 0.52 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at 0.3825 0.5)
		(size 0.52 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at 0.3825 0)
		(size 0.52 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "6" smd roundrect
		(at 0.3825 -0.5)
		(size 0.52 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_SON.3dshapes/Fairchild_MicroPak-6_1.0x1.45mm_P0.5mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
