(footprint "HUSON-3-1EP_2x2mm_P1.3mm_EP1.1x1.6mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "HUSON, 3 Pin, SOT1061 (Ref: https://assets.nexperia.com/documents/data-sheet/PMEG2020CPA.pdf)")
	(tags "huson nolead SOT1061")
	(property "Reference" "REF**"
		(at 0 -2.22 0)
		(layer "F.SilkS")
	)
	(property "Value" "HUSON-3-1EP_2x2mm_P1.3mm_EP1.1x1.6mm"
		(at 0 1.95 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd roundrect
		(at 0.25 -0.42 90)
		(size 0.64 0.97)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 0.25 0.38 90)
		(size 0.64 0.97)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "1" smd roundrect
		(at -0.8 -0.65)
		(size 0.5 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -0.8 0.65)
		(size 0.5 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd rect
		(at 0.25 0)
		(size 1.1 1.6)
		(layers "F.Cu" "F.Mask")
	)
	(pad "3" smd rect
		(at 0.925 0)
		(size 0.25 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_SON.3dshapes/HUSON-3-1EP_2x2mm_P1.3mm_EP1.1x1.6mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
