(footprint "Infineon_PG-TDSON-8_6.15x5.15mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Infineon, PG-TDSON-8, 6.15x5.15x1mm, https://www.infineon.com/dgdl/Infineon-BSC520N15NS3_-DS-v02_02-en.pdf?fileId=db3a30432239cccd0122eee57d9b21a4")
	(tags "Infineon OptiMOS")
	(property "Reference" "REF**"
		(at 0 -3.9 0)
		(layer "F.SilkS")
	)
	(property "Value" "Infineon_PG-TDSON-8_6.15x5.15mm"
		(at 0 3.9 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at -1.9 0.05 90)
		(layer "F.Fab")
	)
	(pad "" smd rect
		(at -0.8 -1.725)
		(size 0.9 0.9)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -0.8 -0.575)
		(size 0.9 0.9)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -0.8 0.575)
		(size 0.9 0.9)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -0.8 1.725)
		(size 0.9 0.9)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.425 -1.725)
		(size 0.9 0.9)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.425 -0.575)
		(size 0.9 0.9)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.425 0.575)
		(size 0.9 0.9)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.425 1.725)
		(size 0.9 0.9)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 1.625 -1.725)
		(size 0.9 0.9)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 1.625 -0.575)
		(size 0.9 0.9)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 1.625 0.575)
		(size 0.9 0.9)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 1.625 1.725)
		(size 0.9 0.9)
		(layers "F.Paste")
	)
	(pad "1" smd roundrect
		(at -2.825 -1.905)
		(size 1.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -2.825 -0.635)
		(size 1.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at -2.825 0.635)
		(size 1.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at -2.825 1.905)
		(size 1.2 0.65)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd rect
		(at 0.675 0)
		(size 4.5 4.7)
		(layers "F.Cu" "F.Mask")
	)
	(pad "5" smd roundrect
		(at 2.925 -1.995)
		(size 1 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at 2.925 -0.665)
		(size 1 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at 2.925 0.665)
		(size 1 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at 2.925 1.995)
		(size 1 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_SON.3dshapes/Infineon_PG-TDSON-8_6.15x5.15mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
