(footprint "Infineon_PG-TISON-8-4"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Infineon, PG-TISON-8-4, 5x6x1.15mm, 1.27mm Pitch, Exposed Paddle, https://www.infineon.com/cms/en/product/packages/PG-TISON/PG-TISON-8-4/")
	(tags "tison")
	(property "Reference" "REF**"
		(at 0 -3.5 0)
		(layer "F.SilkS")
	)
	(property "Value" "Infineon_PG-TISON-8-4"
		(at 0 3.5 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(solder_paste_margin -0.05)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd rect
		(at -2.87 0.635)
		(size 0.7 0.35)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -2.87 0.635)
		(size 0.8 0.45)
		(layers "F.Mask")
	)
	(pad "" smd rect
		(at -2.87 1.905)
		(size 0.7 0.35)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -2.87 1.905)
		(size 0.8 0.45)
		(layers "F.Mask")
	)
	(pad "" smd rect
		(at -1.57 -1.5)
		(size 0.8 0.75)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -1.57 -0.5)
		(size 0.8 0.75)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -1.57 0)
		(size 1 4.25)
		(layers "F.Mask")
	)
	(pad "" smd rect
		(at -1.57 0.5)
		(size 0.8 0.75)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -1.57 1.5)
		(size 0.8 0.75)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0 -1.5)
		(size 0.85 0.75)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0 -0.5)
		(size 0.85 0.75)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0 0.5)
		(size 0.85 0.75)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0 1.5)
		(size 0.85 0.75)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 1.1 -0.315)
		(size 0.85 0.38)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 1.1 0.5)
		(size 0.85 0.75)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 1.1 1.5)
		(size 0.85 0.75)
		(layers "F.Paste")
	)
	(pad "" smd roundrect
		(at 1.92 -1.905)
		(size 0.8 0.35)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 2.87 -1.905)
		(size 0.7 0.35)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "1" smd roundrect
		(at -2.87 -1.905)
		(size 0.8 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -2.87 -0.635)
		(size 0.8 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd custom
		(at -1.57 0)
		(size 1 4.25)
		(layers "F.Cu")
		(zone_connect 2)
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.5 2.13) (xy -1.7 2.13) (xy -1.7 0.41) (xy -0.5 0.41)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "4" smd roundrect
		(at 2.87 1.905)
		(size 0.8 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at 2.87 0.635)
		(size 0.8 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "6" smd roundrect
		(at 2.87 -0.635)
		(size 0.8 0.45)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "7" smd roundrect
		(at 2.37 -1.905)
		(size 1.8 0.45)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "8" smd custom
		(at 0.077 0)
		(size 1.4 4.25)
		(layers "F.Cu" "F.Mask")
		(zone_connect 2)
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy 1.65 2.125) (xy 0.7 2.125) (xy 0.7 -0.675) (xy 1.65 -0.675)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_SON.3dshapes/Infineon_PG-TISON-8-4.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
