(footprint "Infineon_PG-TISON-8-5"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Infineon, PG-TISON-8-5, 8x8x1.1mm, 1mm Pitch, https://www.infineon.com/cms/en/product/packages/PG-TISON/PG-TISON-8-5/")
	(tags "tison")
	(property "Reference" "REF**"
		(at 0 -5.5 0)
		(layer "F.SilkS")
	)
	(property "Value" "Infineon_PG-TISON-8-5"
		(at 0 5.5 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd roundrect
		(at -3.8 -3.5)
		(size 1.2 0.3)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -3.8 -2.5)
		(size 1.2 0.3)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -3.8 -2.5)
		(size 1.2 0.3)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -3.8 -1.5)
		(size 1.2 0.3)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -3.8 -0.5)
		(size 1.2 0.3)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -3.8 0.5)
		(size 1.2 0.3)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -3.8 1.5)
		(size 1.2 0.3)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -3.8 2.5)
		(size 1.2 0.3)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -3.8 3.5)
		(size 1.2 0.3)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -3.49 -3)
		(size 0.5 0.4)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -3.49 3)
		(size 0.5 0.4)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 1.561 -3.6375)
		(size 0.7 1.225)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 1.561 -1.425)
		(size 0.7 1.6)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 1.561 0.4025)
		(size 0.7 0.455)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 1.561 1.9025)
		(size 0.7 0.545)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 1.561 3.6125)
		(size 0.7 1.275)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 2.3795 2.915)
		(size 0.537 2.57)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 2.586 -2.94)
		(size 0.95 2.62)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 3.2795 -0.375)
		(size 0.863 0.5)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 3.2795 1.425)
		(size 0.863 1.5)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 3.2795 3.6125)
		(size 0.863 1.275)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 3.486 -3.6375)
		(size 0.45 1.225)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 3.486 -1.9275)
		(size 0.45 0.595)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 4.111 -2.94)
		(size 0.4 2.62)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 4.111 0.4025)
		(size 0.4 2.055)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 4.111 2.915)
		(size 0.4 2.57)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "1" smd custom
		(at -3.47 -3)
		(size 0.66 1.4)
		(layers "F.Cu" "F.Mask")
		(zone_connect 2)
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.33 0.7) (xy -0.98 0.7) (xy -0.98 0.3) (xy -0.33 0.3) (xy -0.33 -0.3) (xy -0.98 -0.3) (xy -0.98 -0.7)
					(xy 0.33 -0.7)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "2" smd roundrect
		(at -3.8 -1.5)
		(size 1.3 0.4)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at -3.8 -0.5)
		(size 1.3 0.4)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at -3.8 0.5)
		(size 1.3 0.4)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at -3.8 1.5)
		(size 1.3 0.4)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "6" smd custom
		(at -3.47 3)
		(size 0.66 1.4)
		(layers "F.Cu" "F.Mask")
		(zone_connect 2)
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.33 0.7) (xy -0.98 0.7) (xy -0.98 0.3) (xy -0.33 0.3) (xy -0.33 -0.3) (xy -0.98 -0.3) (xy -0.98 -0.7)
					(xy 0.33 -0.7)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "7" smd custom
		(at 2.75 2.965)
		(size 3.5 3.07)
		(layers "F.Cu" "F.Mask")
		(zone_connect 2)
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy 1.75 -1.535) (xy -0.125 -1.535) (xy -0.125 -3.595) (xy 0.075 -3.795) (xy 1.75 -3.795)
				)
				(width 0)
				(fill yes)
			)
			(gr_circle
				(center 0.075 -3.595)
				(end 0.275 -3.595)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "8" smd custom
		(at 2.75 -2.965)
		(size 3.5 3.07)
		(layers "F.Cu" "F.Mask")
		(zone_connect 2)
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.625 3.595) (xy -0.825 3.795) (xy -1.75 3.795) (xy -1.75 1.535) (xy -0.625 1.535)
				)
				(width 0)
				(fill yes)
			)
			(gr_circle
				(center -0.825 3.595)
				(end -0.625 3.595)
				(width 0)
				(fill yes)
			)
		)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_SON.3dshapes/Infineon_PG-TISON-8-5.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
