(footprint "ST_PowerFLAT-6L_5x6mm_P1.27mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Thermally-enhanced 5x6mm 6-pin package, https://www.st.com/resource/en/datasheet/stl40dn3llh5.pdf")
	(tags "PowerFLAT5x6")
	(property "Reference" "REF**"
		(at 0 -3.75 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "ST_PowerFLAT-6L_5x6mm_P1.27mm"
		(at 0 3.8 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "" smd roundrect
		(at -0.175 -1.25 270)
		(size 1.68 1.68)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -0.175 1.25 270)
		(size 1.68 1.68)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 1.775 -1.25 270)
		(size 1.68 1.68)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at 1.775 1.25 270)
		(size 1.68 1.68)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "1" smd roundrect
		(at -2.675 -1.905 270)
		(size 0.65 1.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "2" smd roundrect
		(at -2.675 -0.635 270)
		(size 0.65 1.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "3" smd roundrect
		(at -2.675 0.635 270)
		(size 0.65 1.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "4" smd roundrect
		(at -2.675 1.905 270)
		(size 0.65 1.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "5" smd custom
		(at 0.665 1.25 270)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask")
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.3 -2.635) (xy -0.3 -2.085) (xy 0.325 -2.085) (xy 0.325 -2.635) (xy 1.05 -2.635) (xy 1.05 -1.625)
					(xy 1.45 -1.625) (xy 1.45 -0.825) (xy 1.05 -0.825) (xy 1.05 0.825) (xy 1.45 0.825) (xy 1.45 1.625)
					(xy 1.05 1.625) (xy 1.05 1.815) (xy -1.05 1.815) (xy -1.05 -2.635)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "7" smd custom
		(at 0.665 -1.25 270)
		(size 0.5 0.5)
		(layers "F.Cu" "F.Mask")
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.3 -2.635) (xy 0.3 -2.085) (xy -0.325 -2.085) (xy -0.325 -2.635) (xy -1.05 -2.635) (xy -1.05 -1.625)
					(xy -1.45 -1.625) (xy -1.45 -0.825) (xy -1.05 -0.825) (xy -1.05 0.825) (xy -1.45 0.825) (xy -1.45 1.625)
					(xy -1.05 1.625) (xy -1.05 1.815) (xy 1.05 1.815) (xy 1.05 -2.635)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_SON.3dshapes/ST_PowerFLAT-6L_5x6mm_P1.27mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
