(footprint "ST_PowerFLAT_HV-5_8x8mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "High-Voltage 5-pin package, https://www.st.com/resource/en/datasheet/sctl35n65g2v.pdf")
	(tags "PowerFLAT8x8")
	(property "Reference" "REF**"
		(at 0 -4.8 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "ST_PowerFLAT_HV-5_8x8mm"
		(at 0 4.95 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -3.675 -3)
		(size 1.05 1.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2380952381)
		(thermal_bridge_angle 45)
	)
	(pad "2" smd roundrect
		(at -3.675 -1 180)
		(size 1.05 1.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2380952381)
		(thermal_bridge_angle 45)
	)
	(pad "3" smd roundrect
		(at -3.675 1)
		(size 1.05 1.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2380952381)
		(thermal_bridge_angle 45)
	)
	(pad "4" smd roundrect
		(at -3.675 3)
		(size 1.05 1.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2380952381)
		(thermal_bridge_angle 45)
	)
	(pad "5" smd roundrect
		(at 1.825 0)
		(size 4.75 7.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.05263157895)
		(thermal_bridge_angle 45)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_SON.3dshapes/ST_PowerFLAT_HV-5_8x8mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
