(footprint "ST_PowerFLAT_HV-8_5x6mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "High-Voltage 8-pin package, https://www.st.com/resource/en/datasheet/sgt65r65al.pdf")
	(tags "PowerFLAT5x6")
	(property "Reference" "REF**"
		(at 0 -3.85 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "ST_PowerFLAT_HV-8_5x6mm"
		(at 0 4.95 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(net_tie_pad_groups "1,2")
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "" smd roundrect
		(at -2.855 -1.9049)
		(size 0.78 0.5)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -1.495 -2.04)
		(size 1.285 1.22)
		(layers "F.Paste")
		(roundrect_rratio 0.2049180328)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -1.495 -0.68)
		(size 1.285 1.22)
		(layers "F.Paste")
		(roundrect_rratio 0.2049180328)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -1.495 0.68)
		(size 1.285 1.22)
		(layers "F.Paste")
		(roundrect_rratio 0.2049180328)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -1.492 2.04)
		(size 1.285 1.22)
		(layers "F.Paste")
		(roundrect_rratio 0.2049180328)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -0.07 -2.04)
		(size 1.285 1.22)
		(layers "F.Paste")
		(roundrect_rratio 0.2049180328)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -0.07 -0.68)
		(size 1.285 1.22)
		(layers "F.Paste")
		(roundrect_rratio 0.2049180328)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -0.07 0.68)
		(size 1.285 1.22)
		(layers "F.Paste")
		(roundrect_rratio 0.2049180328)
		(thermal_bridge_angle 45)
	)
	(pad "" smd roundrect
		(at -0.067 2.04)
		(size 1.285 1.22)
		(layers "F.Paste")
		(roundrect_rratio 0.2049180328)
		(thermal_bridge_angle 45)
	)
	(pad "1" smd custom
		(at -2.855 -1.9049)
		(size 0.78 0.5)
		(property pad_prop_heatsink)
		(layers "F.Cu" "F.Mask")
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(arc
						(start -0.265 -0.7951)
						(mid -0.353388 -0.758488)
						(end -0.39 -0.6701)
					)
					(arc
						(start -0.39 1.3899)
						(mid -0.353388 1.478288)
						(end -0.265 1.5149)
					)
					(arc
						(start 0.035 1.5149)
						(mid 0.123388 1.551512)
						(end 0.16 1.6399)
					)
					(arc
						(start 0.16 1.8799)
						(mid 0.196612 1.968288)
						(end 0.285 2.0049)
					)
					(arc
						(start 0.545 2.0049)
						(mid 0.633388 2.041512)
						(end 0.67 2.1299)
					)
					(arc
						(start 0.67 4.4799)
						(mid 0.706612 4.568288)
						(end 0.795 4.6049)
					)
					(arc
						(start 3.355 4.6049)
						(mid 3.443388 4.568288)
						(end 3.48 4.4799)
					)
					(arc
						(start 3.48 -0.6701)
						(mid 3.443388 -0.758488)
						(end 3.355 -0.7951)
					)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "2" smd roundrect
		(at -2.855 -0.6349)
		(size 0.78 0.5)
		(property pad_prop_heatsink)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "3" smd roundrect
		(at -2.855 0.635)
		(size 0.78 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "4" smd roundrect
		(at -2.855 1.905)
		(size 0.78 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "5" smd roundrect
		(at 2.855 1.905)
		(size 0.78 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "6" smd roundrect
		(at 2.855 0.635)
		(size 0.78 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "7" smd roundrect
		(at 2.855 -0.635)
		(size 0.78 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(pad "8" smd roundrect
		(at 2.855 -1.905)
		(size 0.78 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(thermal_bridge_angle 45)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_SON.3dshapes/ST_PowerFLAT_HV-8_5x6mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
