(footprint "Texas_DPY0002A_0.6x1mm_P0.65mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "X1SON 2 pin 0.6x1mm 0.375mm height package, https://www.ti.com/lit/ml/mpss034c/mpss034c.pdf, https://www.ti.com/lit/ds/symlink/tpd6e05u06.pdf")
	(tags "X1SON")
	(property "Reference" "REF**"
		(at 0 -1.25 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "Texas_DPY0002A_0.6x1mm_P0.65mm"
		(at 0 1.25 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -0.35 0)
		(size 0.3 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at 0.35 0)
		(size 0.3 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_SON.3dshapes/Texas_DPY0002A_0.6x1mm_P0.65mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
