(footprint "Texas_DQX002A"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Texas DQX - 2pin WSON, 2.5x1.7mm body, 0.8mm height. https://www.ti.com/lit/ds/symlink/lmt01.pdf")
	(tags "WSON-2 DQX")
	(property "Reference" "REF**"
		(at 0 -2 0)
		(layer "F.SilkS")
	)
	(property "Value" "Texas_DQX002A"
		(at 0 2 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd custom
		(at -0.85 0 90)
		(size 0.001 0.001)
		(layers "F.Cu" "F.Mask")
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.3 0.55) (xy 0.3 0.55) (xy 0.3 -0.55) (xy 0.15 -0.55) (xy 0.15 -0.2) (xy -0.15 -0.2) (xy -0.15 -0.55)
					(xy -0.3 -0.55)
				)
				(width 0.1)
				(fill yes)
			)
		)
	)
	(pad "2" smd custom
		(at 0.85 0 270)
		(size 0.001 0.001)
		(layers "F.Cu" "F.Mask")
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.3 0.55) (xy 0.3 0.55) (xy 0.3 -0.55) (xy 0.15 -0.55) (xy 0.15 -0.2) (xy -0.15 -0.2) (xy -0.15 -0.55)
					(xy -0.3 -0.55)
				)
				(width 0.1)
				(fill yes)
			)
		)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_SON.3dshapes/Texas_DQX002A.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
