(footprint "Texas_DRC0010J"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Texas DRC0010J, VSON10 3x3mm Body, 0.5mm Pitch,  http://www.ti.com/lit/ds/symlink/tps63000.pdf")
	(tags "Texas VSON10 3x3mm")
	(property "Reference" "REF**"
		(at 0.02032 -2.7 0)
		(layer "F.SilkS")
	)
	(property "Value" "Texas_DRC0010J"
		(at 0.02032 2.8 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd roundrect
		(at -0.25 -1.53)
		(size 0.25 0.34)
		(layers "F.Paste")
		(roundrect_rratio 0.1)
		(zone_connect 0)
	)
	(pad "" smd roundrect
		(at -0.25 1.53)
		(size 0.25 0.34)
		(layers "F.Paste")
		(roundrect_rratio 0.1)
		(zone_connect 0)
	)
	(pad "" smd roundrect
		(at 0 -0.63)
		(size 1.5 1.06)
		(layers "F.Paste")
		(roundrect_rratio 0.1)
		(zone_connect 0)
	)
	(pad "" smd roundrect
		(at 0 0.63)
		(size 1.5 1.06)
		(layers "F.Paste")
		(roundrect_rratio 0.1)
		(zone_connect 0)
	)
	(pad "" smd roundrect
		(at 0.25 -1.53)
		(size 0.25 0.34)
		(layers "F.Paste")
		(roundrect_rratio 0.1)
		(zone_connect 0)
	)
	(pad "" smd roundrect
		(at 0.25 1.53)
		(size 0.25 0.34)
		(layers "F.Paste")
		(roundrect_rratio 0.1)
		(zone_connect 0)
	)
	(pad "1" smd roundrect
		(at -1.4 -1)
		(size 0.6 0.24)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -1.4 -0.5)
		(size 0.6 0.24)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at -1.4 0)
		(size 0.6 0.24)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at -1.4 0.5)
		(size 0.6 0.24)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at -1.4 1)
		(size 0.6 0.24)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "6" smd roundrect
		(at 1.4 1)
		(size 0.6 0.24)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "7" smd roundrect
		(at 1.4 0.5)
		(size 0.6 0.24)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "8" smd roundrect
		(at 1.4 0)
		(size 0.6 0.24)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "9" smd roundrect
		(at 1.4 -0.5)
		(size 0.6 0.24)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "10" smd roundrect
		(at 1.4 -1)
		(size 0.6 0.24)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "11" smd custom
		(at 0 0)
		(size 1.65 2.4)
		(layers "F.Cu" "F.Mask")
		(zone_connect 0)
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.125 -1.1) (xy 0.125 -1.1) (xy 0.125 -1.7) (xy 0.375 -1.7) (xy 0.375 1.7) (xy 0.125 1.7)
					(xy 0.125 1.1) (xy -0.125 1.1) (xy -0.125 1.7) (xy -0.375 1.7) (xy -0.375 -1.7) (xy -0.125 -1.7)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_SON.3dshapes/Texas_DRC0010J.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
