(footprint "Texas_S-PDSO-N12"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "http://www.ti.com/lit/ds/symlink/bq27441-g1.pdf")
	(tags "SON thermal pads")
	(property "Reference" "REF**"
		(at -0.000701 -2.517393 0)
		(layer "F.SilkS")
	)
	(property "Value" "Texas_S-PDSO-N12"
		(at -0.000701 2.852607 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at -0.000701 0.002607 0)
		(layer "F.Fab")
	)
	(pad "" smd roundrect
		(at -1.125 -1.2625)
		(size 0.2 0.375)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -1.125 1.2625)
		(size 0.2 0.375)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -0.64 0)
		(size 1.08 1.75)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 0.64 0)
		(size 1.08 1.75)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 1.125 -1.2625)
		(size 0.2 0.375)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 1.125 1.2625)
		(size 0.2 0.375)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "1" smd roundrect
		(at -1.9 -1)
		(size 0.6 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(chamfer_ratio 0.2)
		(chamfer)
	)
	(pad "2" smd roundrect
		(at -1.9 -0.6)
		(size 0.6 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(chamfer_ratio 0.2)
		(chamfer)
	)
	(pad "3" smd roundrect
		(at -1.9 -0.2)
		(size 0.6 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(chamfer_ratio 0.2)
		(chamfer)
	)
	(pad "4" smd roundrect
		(at -1.9 0.2)
		(size 0.6 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(chamfer_ratio 0.2)
		(chamfer)
	)
	(pad "5" smd roundrect
		(at -1.9 0.6)
		(size 0.6 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(chamfer_ratio 0.2)
		(chamfer)
	)
	(pad "6" smd roundrect
		(at -1.9 1)
		(size 0.6 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(chamfer_ratio 0.2)
		(chamfer)
	)
	(pad "7" smd roundrect
		(at 1.9 1)
		(size 0.6 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(chamfer_ratio 0.2)
		(chamfer)
	)
	(pad "8" smd roundrect
		(at 1.9 0.6)
		(size 0.6 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(chamfer_ratio 0.2)
		(chamfer)
	)
	(pad "9" smd roundrect
		(at 1.9 0.2)
		(size 0.6 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(chamfer_ratio 0.2)
		(chamfer)
	)
	(pad "10" smd roundrect
		(at 1.9 -0.2)
		(size 0.6 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(chamfer_ratio 0.2)
		(chamfer)
	)
	(pad "11" smd roundrect
		(at 1.9 -0.6)
		(size 0.6 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(chamfer_ratio 0.2)
		(chamfer)
	)
	(pad "12" smd roundrect
		(at 1.9 -1)
		(size 0.6 0.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(chamfer_ratio 0.2)
		(chamfer)
	)
	(pad "13" smd roundrect
		(at -1.125 -1.1875 270)
		(size 0.525 0.2)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "13" smd roundrect
		(at -1.125 1.1875 270)
		(size 0.525 0.2)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "13" thru_hole circle
		(at -0.975 0)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "13" thru_hole circle
		(at 0 -0.725)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "13" thru_hole circle
		(at 0 0)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "13" smd rect
		(at 0 0 270)
		(size 1.95 2.45)
		(layers "F.Cu" "F.Mask")
	)
	(pad "13" thru_hole circle
		(at 0 0.725)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "13" thru_hole circle
		(at 0.975 0)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "13" smd roundrect
		(at 1.125 -1.1875 270)
		(size 0.525 0.2)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "13" smd roundrect
		(at 1.125 1.1875 270)
		(size 0.525 0.2)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_SON.3dshapes/Texas_S-PDSO-N12.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
