(footprint "Texas_S-PVSON-N8"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "8-Lead Plastic VSON, 3x3mm Body, 0.65mm Pitch, S-PVSON-N8, http://www.ti.com/lit/ds/symlink/opa2333.pdf")
	(tags "DFN 0.65 S-PVSON-N8")
	(property "Reference" "REF**"
		(at 0 -2.5 0)
		(layer "F.SilkS")
	)
	(property "Value" "Texas_S-PVSON-N8"
		(at 0 2.6 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -1.75 -0.975)
		(size 0.3 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.05)
	)
	(pad "1" smd oval
		(at -1.55 -0.975)
		(size 0.65 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.05)
	)
	(pad "2" smd rect
		(at -1.75 -0.325)
		(size 0.3 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.05)
	)
	(pad "2" smd oval
		(at -1.55 -0.325)
		(size 0.65 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.05)
	)
	(pad "3" smd rect
		(at -1.75 0.325)
		(size 0.3 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.05)
	)
	(pad "3" smd oval
		(at -1.55 0.325)
		(size 0.65 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.05)
	)
	(pad "4" smd rect
		(at -1.75 0.975)
		(size 0.3 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.05)
	)
	(pad "4" smd oval
		(at -1.55 0.975)
		(size 0.65 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.05)
	)
	(pad "5" smd oval
		(at 1.55 0.975)
		(size 0.65 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.05)
	)
	(pad "5" smd rect
		(at 1.75 0.975)
		(size 0.3 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.05)
	)
	(pad "6" smd oval
		(at 1.55 0.325)
		(size 0.65 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.05)
	)
	(pad "6" smd rect
		(at 1.75 0.325)
		(size 0.3 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.05)
	)
	(pad "7" smd oval
		(at 1.55 -0.325)
		(size 0.65 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.05)
	)
	(pad "7" smd rect
		(at 1.75 -0.325)
		(size 0.3 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.05)
	)
	(pad "8" smd oval
		(at 1.55 -0.975)
		(size 0.65 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.05)
	)
	(pad "8" smd rect
		(at 1.75 -0.975)
		(size 0.3 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.05)
	)
	(pad "9" smd rect
		(at -0.45 -0.625)
		(size 0.65 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at -0.45 0.625)
		(size 0.65 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at 0 0)
		(size 1.65 2.4)
		(layers "F.Cu" "F.Mask")
	)
	(pad "9" smd rect
		(at 0.45 -0.625)
		(size 0.65 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at 0.45 0.625)
		(size 0.65 1)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_SON.3dshapes/Texas_S-PVSON-N8.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
