(footprint "Texas_S-PWSON-N10_ThermalVias"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "3x3mm Body, 0.5mm Pitch, S-PWSON-N10, DSC, http://www.ti.com/lit/ds/symlink/tps63060.pdf")
	(tags "0.5 S-PWSON-N10 DSC")
	(property "Reference" "REF**"
		(at 0 -2.8 0)
		(layer "F.SilkS")
	)
	(property "Value" "Texas_S-PWSON-N10_ThermalVias"
		(at 0 2.8 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -1.76 -1)
		(size 0.28 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.025)
	)
	(pad "1" smd oval
		(at -1.475 -1)
		(size 0.85 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.025)
	)
	(pad "2" smd rect
		(at -1.76 -0.5)
		(size 0.28 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.025)
	)
	(pad "2" smd oval
		(at -1.475 -0.5)
		(size 0.85 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.025)
	)
	(pad "3" smd rect
		(at -1.76 0)
		(size 0.28 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.025)
	)
	(pad "3" smd oval
		(at -1.475 0)
		(size 0.85 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.025)
	)
	(pad "4" smd rect
		(at -1.76 0.5)
		(size 0.28 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.025)
	)
	(pad "4" smd oval
		(at -1.475 0.5)
		(size 0.85 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.025)
	)
	(pad "5" smd rect
		(at -1.76 1)
		(size 0.28 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.025)
	)
	(pad "5" smd oval
		(at -1.475 1)
		(size 0.85 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.025)
	)
	(pad "6" smd oval
		(at 1.475 1)
		(size 0.85 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.025)
	)
	(pad "6" smd rect
		(at 1.76 1)
		(size 0.28 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.025)
	)
	(pad "7" smd oval
		(at 1.475 0.5)
		(size 0.85 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.025)
	)
	(pad "7" smd rect
		(at 1.76 0.5)
		(size 0.28 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.025)
	)
	(pad "8" smd oval
		(at 1.475 0)
		(size 0.85 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.025)
	)
	(pad "8" smd rect
		(at 1.76 0)
		(size 0.28 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.025)
	)
	(pad "9" smd oval
		(at 1.475 -0.5)
		(size 0.85 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.025)
	)
	(pad "9" smd rect
		(at 1.76 -0.5)
		(size 0.28 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.025)
	)
	(pad "10" smd oval
		(at 1.475 -1)
		(size 0.85 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.025)
	)
	(pad "10" smd rect
		(at 1.76 -1)
		(size 0.28 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.025)
	)
	(pad "11" smd rect
		(at -0.6 -1.425)
		(size 0.23 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at -0.6 -1.425)
		(size 0.25 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.05)
	)
	(pad "11" smd rect
		(at -0.6 1.425)
		(size 0.23 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at -0.6 1.425)
		(size 0.25 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.05)
	)
	(pad "11" thru_hole circle
		(at -0.5 -0.5)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at -0.5 0.5)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" smd rect
		(at -0.435 -0.56)
		(size 0.65 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at -0.435 0.56)
		(size 0.65 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at -0.2 -1.425)
		(size 0.23 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at -0.2 -1.425)
		(size 0.25 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.05)
	)
	(pad "11" smd rect
		(at -0.2 1.425)
		(size 0.23 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at -0.2 1.425)
		(size 0.25 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.05)
	)
	(pad "11" smd rect
		(at -0.001 0)
		(size 2.3 2.3)
		(layers "B.Cu")
	)
	(pad "11" thru_hole circle
		(at 0 0)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" smd rect
		(at 0 0)
		(size 1.7 2.15)
		(layers "F.Cu" "F.Mask")
	)
	(pad "11" smd rect
		(at 0.2 -1.425)
		(size 0.23 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at 0.2 -1.425)
		(size 0.25 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.05)
	)
	(pad "11" smd rect
		(at 0.2 1.425)
		(size 0.23 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at 0.2 1.425)
		(size 0.25 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.05)
	)
	(pad "11" smd rect
		(at 0.435 -0.56)
		(size 0.65 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at 0.435 0.56)
		(size 0.65 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" thru_hole circle
		(at 0.5 -0.5)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" thru_hole circle
		(at 0.5 0.5)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "11" smd rect
		(at 0.6 -1.425)
		(size 0.23 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at 0.6 -1.425)
		(size 0.25 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.05)
	)
	(pad "11" smd rect
		(at 0.6 1.425)
		(size 0.23 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at 0.6 1.425)
		(size 0.25 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin -0.05)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_SON.3dshapes/Texas_S-PWSON-N10.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
