(footprint "Texas_USON-6_1x1.45mm_P0.5mm_SMD"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "USON, 6 Pin (https://www.ti.com/lit/ds/symlink/sn74auc1g04.pdf#page=24), Solder Mask Defined")
	(tags "USON NoLead DRY0006A")
	(property "Reference" "REF**"
		(at 0 -2 0)
		(layer "F.SilkS")
	)
	(property "Value" "Texas_USON-6_1x1.45mm_P0.5mm_SMD"
		(at 0 1.68 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(solder_mask_margin -0.05)
	(solder_paste_margin -0.05)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 90)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -0.275 -0.5)
		(size 0.45 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.3333333333)
	)
	(pad "2" smd roundrect
		(at -0.3 0)
		(size 0.4 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.3333333333)
	)
	(pad "3" smd roundrect
		(at -0.3 0.5)
		(size 0.4 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.3333333333)
	)
	(pad "4" smd roundrect
		(at 0.3 0.5)
		(size 0.4 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.3333333333)
	)
	(pad "5" smd roundrect
		(at 0.3 0)
		(size 0.4 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.3333333333)
	)
	(pad "6" smd roundrect
		(at 0.3 -0.5)
		(size 0.4 0.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.3333333333)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_SON.3dshapes/USON-6_1x1.45mm_P0.5mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
