(footprint "Texas_X2SON-4_1x1mm_P0.65mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "X2SON 5 pin 1x1mm package, DQN0004A (Reference Datasheet: http://www.ti.com/lit/ds/sbvs193d/sbvs193d.pdf Reference part: TPS383x) [StepUp generated footprint]")
	(tags "X2SON")
	(property "Reference" "REF**"
		(at 0 -1.5 0)
		(layer "F.SilkS")
	)
	(property "Value" "Texas_X2SON-4_1x1mm_P0.65mm"
		(at 0 1.5 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd custom
		(at -0.43 -0.325)
		(size 0.148492 0.148492)
		(layers "F.Mask")
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.18 -0.075) (xy 0 0.105) (xy -0.18 0.105) (xy -0.18 -0.105) (xy 0.18 -0.105)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "" smd custom
		(at -0.43 -0.325)
		(size 0.148492 0.148492)
		(layers "F.Paste")
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.18 -0.075) (xy 0 0.105) (xy -0.22 0.105) (xy -0.22 -0.105) (xy 0.18 -0.105)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "" smd custom
		(at -0.43 0.325)
		(size 0.148492 0.148492)
		(layers "F.Mask")
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.18 0.075) (xy 0.18 0.105) (xy -0.18 0.105) (xy -0.18 -0.105) (xy 0 -0.105)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "" smd custom
		(at -0.43 0.325)
		(size 0.148492 0.148492)
		(layers "F.Paste")
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.18 0.075) (xy 0.18 0.105) (xy -0.22 0.105) (xy -0.22 -0.105) (xy 0 -0.105)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "" smd custom
		(at 0.43 -0.325)
		(size 0.148492 0.148492)
		(layers "F.Mask")
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.18 0.105) (xy 0 0.105) (xy -0.18 -0.075) (xy -0.18 -0.105) (xy 0.18 -0.105)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "" smd custom
		(at 0.43 -0.325)
		(size 0.148492 0.148492)
		(layers "F.Paste")
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.22 0.105) (xy 0 0.105) (xy -0.18 -0.075) (xy -0.18 -0.105) (xy 0.22 -0.105)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "" smd custom
		(at 0.43 0.325)
		(size 0.148492 0.148492)
		(layers "F.Mask")
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.18 0.105) (xy -0.18 0.105) (xy -0.18 0.075) (xy 0 -0.105) (xy 0.18 -0.105)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "" smd custom
		(at 0.43 0.325)
		(size 0.148492 0.148492)
		(layers "F.Paste")
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.22 0.105) (xy -0.18 0.105) (xy -0.18 0.075) (xy 0 -0.105) (xy 0.22 -0.105)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "1" smd custom
		(at -0.43 -0.325)
		(size 0.148492 0.148492)
		(layers "F.Cu")
		(zone_connect 2)
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.23 -0.054289) (xy 0.020711 0.155) (xy -0.23 0.155) (xy -0.23 -0.155) (xy 0.23 -0.155)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "2" smd custom
		(at -0.43 0.325)
		(size 0.148492 0.148492)
		(layers "F.Cu")
		(zone_connect 2)
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.23 0.054289) (xy 0.23 0.155) (xy -0.23 0.155) (xy -0.23 -0.155) (xy 0.020711 -0.155)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "3" smd custom
		(at 0.43 0.325)
		(size 0.148492 0.148492)
		(layers "F.Cu")
		(zone_connect 2)
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.23 0.155) (xy -0.23 0.155) (xy -0.23 0.054289) (xy -0.020711 -0.155) (xy 0.23 -0.155)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "4" smd custom
		(at 0.43 -0.325)
		(size 0.148492 0.148492)
		(layers "F.Cu")
		(zone_connect 2)
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.23 0.155) (xy -0.020711 0.155) (xy -0.23 -0.054289) (xy -0.23 -0.155) (xy 0.23 -0.155)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "5" smd roundrect
		(at 0 0 45)
		(size 0.58 0.58)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.065)
		(solder_paste_margin_ratio -0.00000001)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_SON.3dshapes/Texas_X2SON-4_1x1mm_P0.65mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
