(footprint "Texas_X2SON-5_0.8x0.8mm_P0.48mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "X2SON 5 pin 0.8x0.8mm package (Reference Datasheet: https://www.ti.com/lit/ds/symlink/sn74lvc1g17.pdf#page=39 Reference part: SN74LVC1G17) [StepUp generated footprint]")
	(tags "X2SON DPW0005A")
	(property "Reference" "REF**"
		(at 0 -1.5 0)
		(layer "F.SilkS")
	)
	(property "Value" "Texas_X2SON-5_0.8x0.8mm_P0.48mm"
		(at 0 2 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 1.1 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "" smd custom
		(at -0.39 -0.24)
		(size 0.15 0.15)
		(layers "F.Mask" "F.Paste")
		(zone_connect 0)
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.05 0.11) (xy 0.21 -0.05) (xy 0.21 -0.11) (xy -0.16 -0.11) (xy -0.195 -0.095) (xy -0.21 -0.06)
					(xy -0.21 0.06) (xy -0.195 0.095) (xy -0.16 0.11)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "" smd custom
		(at -0.39 0.24)
		(size 0.05 0.05)
		(layers "F.Mask" "F.Paste")
		(zone_connect 0)
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.16 -0.11) (xy 0.05 -0.11) (xy 0.21 0.05) (xy 0.21 0.11) (xy -0.16 0.11) (xy -0.195 0.095)
					(xy -0.21 0.06) (xy -0.21 -0.06) (xy -0.195 -0.095)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "" smd custom
		(at 0.39 -0.24)
		(size 0.05 0.05)
		(layers "F.Mask" "F.Paste")
		(zone_connect 0)
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.16 0.11) (xy -0.05 0.11) (xy -0.21 -0.05) (xy -0.21 -0.11) (xy 0.16 -0.11) (xy 0.195 -0.095)
					(xy 0.21 -0.06) (xy 0.21 0.06) (xy 0.195 0.095)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "" smd custom
		(at 0.39 0.24)
		(size 0.15 0.15)
		(layers "F.Paste")
		(zone_connect 0)
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.05 -0.11) (xy -0.21 0.05) (xy -0.21 0.11) (xy 0.16 0.11) (xy 0.195 0.095) (xy 0.21 0.06)
					(xy 0.21 -0.06) (xy 0.195 -0.095) (xy 0.16 -0.11)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "1" smd custom
		(at -0.39 -0.24)
		(size 0.15 0.15)
		(layers "F.Cu" "F.Mask")
		(zone_connect 0)
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.071 0.16) (xy 0.26 -0.029) (xy 0.26 -0.16) (xy -0.16 -0.16) (xy -0.21 -0.147) (xy -0.247 -0.11)
					(xy -0.26 -0.06) (xy -0.26 0.06) (xy -0.247 0.11) (xy -0.21 0.147) (xy -0.16 0.16)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "2" smd custom
		(at -0.39 0.24)
		(size 0.05 0.05)
		(layers "F.Cu" "F.Mask")
		(zone_connect 0)
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.21 -0.147) (xy -0.16 -0.16) (xy 0.071 -0.16) (xy 0.26 0.029) (xy 0.26 0.16) (xy -0.16 0.16)
					(xy -0.21 0.147) (xy -0.247 0.11) (xy -0.26 0.06) (xy -0.26 -0.06) (xy -0.247 -0.11)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "3" smd roundrect
		(at 0 0 45)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.2857142857)
		(solder_mask_margin -0.05)
		(solder_paste_margin -0.055)
		(zone_connect 0)
	)
	(pad "4" smd custom
		(at 0.39 0.24)
		(size 0.15 0.15)
		(layers "F.Cu" "F.Mask")
		(zone_connect 0)
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.071 -0.16) (xy -0.26 0.029) (xy -0.26 0.16) (xy 0.16 0.16) (xy 0.21 0.147) (xy 0.247 0.11)
					(xy 0.26 0.06) (xy 0.26 -0.06) (xy 0.247 -0.11) (xy 0.21 -0.147) (xy 0.16 -0.16)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "5" smd custom
		(at 0.39 -0.24)
		(size 0.05 0.05)
		(layers "F.Cu" "F.Mask")
		(zone_connect 0)
		(thermal_bridge_angle 90)
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.21 0.147) (xy 0.16 0.16) (xy -0.071 0.16) (xy -0.26 -0.029) (xy -0.26 -0.16) (xy 0.16 -0.16)
					(xy 0.21 -0.147) (xy 0.247 -0.11) (xy 0.26 -0.06) (xy 0.26 0.06) (xy 0.247 0.11)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_SON.3dshapes/Texas_X2SON-5_0.8x0.8mm_P0.48mm_Via.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
