(footprint "VSON-10-1EP_3x3mm_P0.5mm_EP1.65x2.4mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "VSON 10 Thermal on 11 3x3mm Pitch 0.5mm http://chip.tomsk.ru/chip/chipdoc.nsf/Package/D8A64DD165C2AAD9472579400024FC41!OpenDocument")
	(tags "VSON 10 Thermal on 11 3x3mm Pitch 0.5mm")
	(property "Reference" "REF**"
		(at 0 -2.9 0)
		(layer "F.SilkS")
	)
	(property "Value" "VSON-10-1EP_3x3mm_P0.5mm_EP1.65x2.4mm"
		(at 0 3 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd rect
		(at -0.4125 -0.8)
		(size 0.64 0.64)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -0.4125 0)
		(size 0.64 0.64)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -0.4125 0.8)
		(size 0.64 0.64)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.4125 -0.8)
		(size 0.64 0.64)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.4125 0)
		(size 0.64 0.64)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.4125 0.8)
		(size 0.64 0.64)
		(layers "F.Paste")
	)
	(pad "1" smd roundrect
		(at -1.475 -1)
		(size 0.85 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -1.475 -0.5)
		(size 0.85 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at -1.475 0)
		(size 0.85 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at -1.475 0.5)
		(size 0.85 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at -1.475 1)
		(size 0.85 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "6" smd roundrect
		(at 1.475 1)
		(size 0.85 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "7" smd roundrect
		(at 1.475 0.5)
		(size 0.85 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "8" smd roundrect
		(at 1.475 0)
		(size 0.85 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "9" smd roundrect
		(at 1.475 -0.5)
		(size 0.85 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "10" smd roundrect
		(at 1.475 -1)
		(size 0.85 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "11" smd rect
		(at -0.25 -1.55)
		(size 0.28 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at -0.25 1.55)
		(size 0.28 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at 0 0)
		(size 1.65 2.4)
		(layers "F.Cu" "F.Mask")
	)
	(pad "11" smd rect
		(at 0.25 -1.55)
		(size 0.28 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at 0.25 1.55)
		(size 0.28 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_SON.3dshapes/VSON-10-1EP_3x3mm_P0.5mm_EP1.65x2.4mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
