(footprint "VSON-14-1EP_3x4.45mm_P0.65mm_EP1.6x4.2mm_ThermalVias"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "VSON, 14 Pin (https://www.ti.com/lit/ds/symlink/lp8868x-q1.pdf#page=45), generated with kicad-footprint-generator ipc_noLead_generator.py")
	(tags "VSON NoLead")
	(property "Reference" "REF**"
		(at 0 -3.18 0)
		(layer "F.SilkS")
	)
	(property "Value" "VSON-14-1EP_3x4.45mm_P0.65mm_EP1.6x4.2mm_ThermalVias"
		(at 0 3.18 0)
		(layer "F.Fab")
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 90)
		(layer "F.Fab")
	)
	(pad "" smd custom
		(at -0.5875 -1.8)
		(size 0.162868 0.162868)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.127122 -0.197667)
					(xy 0.127122 -0.197667)
					(xy 0.127122 -0.030685)
					(xy -0.10123 0.197667)
					(xy -0.127122 0.197667)
				)
				(width 0.088402)
			)
		)
	)
	(pad "" smd custom
		(at -0.5875 -0.75)
		(size 0.224527 0.224527)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.085661 -0.519008)
					(xy -0.031205 -0.519008)
					(xy 0.085661 -0.402141)
					(xy 0.085661 0.402141)
					(xy -0.031205 0.519008)
					(xy -0.085661 0.519008)
				)
				(width 0.171323)
			)
		)
	)
	(pad "" smd custom
		(at -0.5875 0.75)
		(size 0.224527 0.224527)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.085661 -0.519008)
					(xy -0.031205 -0.519008)
					(xy 0.085661 -0.402141)
					(xy 0.085661 0.402141)
					(xy -0.031205 0.519008)
					(xy -0.085661 0.519008)
				)
				(width 0.171323)
			)
		)
	)
	(pad "" smd custom
		(at -0.5875 1.8)
		(size 0.162868 0.162868)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.127122 -0.197667)
					(xy -0.10123 -0.197667)
					(xy 0.127122 0.030685)
					(xy 0.127122 0.197667)
					(xy -0.127122 0.197667)
				)
				(width 0.088402)
			)
		)
	)
	(pad "" smd custom
		(at 0 -1.8)
		(size 0.326223 0.326223)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.181401 -0.120934)
					(xy 0.181401 -0.120934)
					(xy 0.181401 -0.030981)
					(xy 0.029486 0.120934)
					(xy -0.029486 0.120934)
					(xy -0.181401 -0.030981)
				)
				(width 0.241868)
			)
		)
	)
	(pad "" smd custom
		(at 0 -0.75)
		(size 0.508816 0.508816)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.206481 -0.429408)
					(xy -0.127073 -0.508816)
					(xy 0.127073 -0.508816)
					(xy 0.206481 -0.429408)
					(xy 0.206481 0.429408)
					(xy 0.127073 0.508816)
					(xy -0.127073 0.508816)
					(xy -0.206481 0.429408)
				)
				(width 0.191707)
			)
		)
	)
	(pad "" smd custom
		(at 0 0.75)
		(size 0.508816 0.508816)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.206481 -0.429408)
					(xy -0.127073 -0.508816)
					(xy 0.127073 -0.508816)
					(xy 0.206481 -0.429408)
					(xy 0.206481 0.429408)
					(xy 0.127073 0.508816)
					(xy -0.127073 0.508816)
					(xy -0.206481 0.429408)
				)
				(width 0.191707)
			)
		)
	)
	(pad "" smd custom
		(at 0 1.8)
		(size 0.326223 0.326223)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.181401 0.030981)
					(xy -0.029486 -0.120934)
					(xy 0.029486 -0.120934)
					(xy 0.181401 0.030981)
					(xy 0.181401 0.120934)
					(xy -0.181401 0.120934)
				)
				(width 0.241868)
			)
		)
	)
	(pad "" smd custom
		(at 0.5875 -1.8)
		(size 0.162868 0.162868)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.127122 -0.197667)
					(xy 0.127122 -0.197667)
					(xy 0.127122 0.197667)
					(xy 0.10123 0.197667)
					(xy -0.127122 -0.030685)
				)
				(width 0.088402)
			)
		)
	)
	(pad "" smd custom
		(at 0.5875 -0.75)
		(size 0.224527 0.224527)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.085661 -0.402141)
					(xy 0.031205 -0.519008)
					(xy 0.085661 -0.519008)
					(xy 0.085661 0.519008)
					(xy 0.031205 0.519008)
					(xy -0.085661 0.402141)
				)
				(width 0.171323)
			)
		)
	)
	(pad "" smd custom
		(at 0.5875 0.75)
		(size 0.224527 0.224527)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.085661 -0.402141)
					(xy 0.031205 -0.519008)
					(xy 0.085661 -0.519008)
					(xy 0.085661 0.519008)
					(xy 0.031205 0.519008)
					(xy -0.085661 0.402141)
				)
				(width 0.171323)
			)
		)
	)
	(pad "" smd custom
		(at 0.5875 1.8)
		(size 0.162868 0.162868)
		(layers "F.Paste")
		(options
			(clearance outline)
			(anchor circle)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.127122 0.030685)
					(xy 0.10123 -0.197667)
					(xy 0.127122 -0.197667)
					(xy 0.127122 0.197667)
					(xy -0.127122 0.197667)
				)
				(width 0.088402)
			)
		)
	)
	(pad "1" smd roundrect
		(at -1.45 -1.95)
		(size 0.85 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -1.45 -1.3)
		(size 0.85 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at -1.45 -0.65)
		(size 0.85 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at -1.45 0)
		(size 0.85 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at -1.45 0.65)
		(size 0.85 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "6" smd roundrect
		(at -1.45 1.3)
		(size 0.85 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "7" smd roundrect
		(at -1.45 1.95)
		(size 0.85 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "8" smd roundrect
		(at 1.45 1.95)
		(size 0.85 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "9" smd roundrect
		(at 1.45 1.3)
		(size 0.85 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "10" smd roundrect
		(at 1.45 0.65)
		(size 0.85 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "11" smd roundrect
		(at 1.45 0)
		(size 0.85 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "12" smd roundrect
		(at 1.45 -0.65)
		(size 0.85 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "13" smd roundrect
		(at 1.45 -1.3)
		(size 0.85 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "14" smd roundrect
		(at 1.45 -1.95)
		(size 0.85 0.3)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "15" thru_hole circle
		(at -0.375 -1.5)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "15" thru_hole circle
		(at -0.375 0)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "15" thru_hole circle
		(at -0.375 1.5)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "15" smd rect
		(at 0 0)
		(size 1.25 3.5)
		(property pad_prop_heatsink)
		(layers "B.Cu")
		(zone_connect 2)
	)
	(pad "15" smd rect
		(at 0 0)
		(size 1.6 4.2)
		(property pad_prop_heatsink)
		(layers "F.Cu" "F.Mask")
		(zone_connect 2)
	)
	(pad "15" thru_hole circle
		(at 0.375 -1.5)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "15" thru_hole circle
		(at 0.375 0)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "15" thru_hole circle
		(at 0.375 1.5)
		(size 0.5 0.5)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(model "${KICAD9_3DMODEL_DIR}/Package_SON.3dshapes/VSON-14-1EP_3x4.45mm_P0.65mm_EP1.6x4.2mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
