(footprint "VSONP-8-1EP_5x6_P1.27mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "SON, 8-Leads, Body 5x6x1mm, Pitch 1.27mm; (see Texas Instruments CSD18531Q5A http://www.ti.com/lit/ds/symlink/csd18531q5a.pdf)")
	(tags "VSONP 1.27")
	(property "Reference" "REF**"
		(at 0 -3.4 0)
		(layer "F.SilkS")
	)
	(property "Value" "VSONP-8-1EP_5x6_P1.27mm"
		(at 0 3.4 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd rect
		(at -0.7975 -1.095)
		(size 1.235 1.57)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -0.7975 1.095)
		(size 1.235 1.57)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 1.1125 -1.095)
		(size 1.585 1.57)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 1.1125 1.095)
		(size 1.585 1.57)
		(layers "F.Paste")
	)
	(pad "1" smd roundrect
		(at -2.8 -1.905)
		(size 0.7 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_paste_margin_ratio -0.15)
	)
	(pad "1" smd roundrect
		(at -2.8 -0.635)
		(size 0.7 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_paste_margin_ratio -0.15)
	)
	(pad "1" smd roundrect
		(at -2.8 0.635)
		(size 0.7 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_paste_margin_ratio -0.15)
	)
	(pad "2" smd roundrect
		(at -2.8 1.905)
		(size 0.7 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_paste_margin_ratio -0.15)
	)
	(pad "3" smd rect
		(at 0.33 0)
		(size 4.35 4.51)
		(layers "F.Cu" "F.Mask")
		(solder_paste_margin_ratio -0.5)
	)
	(pad "3" smd rect
		(at 2.8 -1.905)
		(size 0.7 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin_ratio -0.15)
	)
	(pad "3" smd rect
		(at 2.8 -0.635)
		(size 0.7 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin_ratio -0.15)
	)
	(pad "3" smd rect
		(at 2.8 0.635)
		(size 0.7 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin_ratio -0.15)
	)
	(pad "3" smd rect
		(at 2.8 1.905)
		(size 0.7 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_paste_margin_ratio -0.15)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_SON.3dshapes/VSONP-8-1EP_5x6_P1.27mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
