(footprint "WSON-14-1EP_4.0x4.0mm_P0.5mm_EP2.6x2.6mm"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "14-Lead Plastic Dual Flat, No Lead Package - 4.0x4.0x0.8 mm Body [WSON], http://www.ti.com/lit/ml/mpds421/mpds421.pdf")
	(tags "NHL014B")
	(property "Reference" "REF**"
		(at 0.027363 -3.153276 0)
		(layer "F.SilkS")
	)
	(property "Value" "WSON-14-1EP_4.0x4.0mm_P0.5mm_EP2.6x2.6mm"
		(at 0 4 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0.05 0.025 0)
		(layer "F.Fab")
	)
	(pad "" smd rect
		(at -0.65 -0.65 270)
		(size 1.05 1.05)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -0.65 0.65 270)
		(size 1.05 1.05)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.65 -0.65 270)
		(size 1.05 1.05)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0.65 0.65 270)
		(size 1.05 1.05)
		(layers "F.Paste")
	)
	(pad "1" smd roundrect
		(at -1.9 -1.5 270)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -1.9 -1 270)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at -1.9 -0.5 270)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at -1.9 0 270)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at -1.9 0.5 270)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "6" smd roundrect
		(at -1.9 1 270)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "7" smd roundrect
		(at -1.9 1.5 270)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "8" smd roundrect
		(at 1.9 1.5 270)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "9" smd roundrect
		(at 1.9 1 270)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "10" smd roundrect
		(at 1.9 0.5 270)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "11" smd roundrect
		(at 1.9 0 270)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "12" smd roundrect
		(at 1.9 -0.5 270)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "13" smd roundrect
		(at 1.9 -1 270)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "14" smd roundrect
		(at 1.9 -1.5 270)
		(size 0.25 0.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "15" smd rect
		(at 0.025 0 270)
		(size 2.6 2.6)
		(layers "F.Cu" "F.Mask")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_SON.3dshapes/WSON-14-1EP_4.0x4.0mm_P0.5mm_EP2.6x2.6mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
