(footprint "ATPAK-2"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "ATPAK SMD package, http://www.onsemi.com/pub/Collateral/ENA2192-D.PDF")
	(tags "ATPAK ")
	(property "Reference" "REF**"
		(at 0 -4.5 0)
		(layer "F.SilkS")
	)
	(property "Value" "ATPAK-2"
		(at 0 4.5 0)
		(layer "F.Fab")
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -4.95 -2.3)
		(size 1.6 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.166667)
	)
	(pad "2" smd roundrect
		(at -0.55 -1.7)
		(size 3.2 3.1)
		(layers "F.Cu" "F.Paste")
		(roundrect_rratio 0.080645)
	)
	(pad "2" smd roundrect
		(at -0.55 1.7)
		(size 3.2 3.1)
		(layers "F.Cu" "F.Paste")
		(roundrect_rratio 0.080645)
	)
	(pad "2" smd roundrect
		(at 1.2 0)
		(size 6.7 6.5)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.038462)
	)
	(pad "2" smd roundrect
		(at 2.95 -1.7)
		(size 3.2 3.1)
		(layers "F.Cu" "F.Paste")
		(roundrect_rratio 0.080645)
	)
	(pad "2" smd roundrect
		(at 2.95 1.7)
		(size 3.2 3.1)
		(layers "F.Cu" "F.Paste")
		(roundrect_rratio 0.080645)
	)
	(pad "3" smd roundrect
		(at -4.95 2.3)
		(size 1.6 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.166667)
	)
	(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/ATPAK-2.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
