(footprint "Analog_KS-4"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Analog Devices KS-4, http://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/sc70ks/ks_4.pdf")
	(tags "Analog Devices KS-4 (like EIAJ SC-82)")
	(property "Reference" "REF**"
		(at 0 -2.2 0)
		(layer "F.SilkS")
	)
	(property "Value" "Analog_KS-4"
		(at 0 2 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 90)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -0.825 -0.65)
		(size 0.75 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -0.825 0.5)
		(size 0.75 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at 0.825 0.65)
		(size 0.75 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at 0.825 -0.65)
		(size 0.75 0.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/Analog_KS-4.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
