(footprint "HVSOF5"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "HVSOF5, http://rohmfs.rohm.com/en/techdata_basic/ic/package/hvsof5_1-e.pdf, http://rohmfs.rohm.com/en/products/databook/datasheet/ic/sensor/hall/bu52001gul-e.pdf")
	(tags "HVSOF5")
	(property "Reference" "REF**"
		(at 0 -1.8 0)
		(layer "F.SilkS")
	)
	(property "Value" "HVSOF5"
		(at 0 1.9 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 90)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -0.675 -0.5)
		(size 0.35 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd custom
		(at 0 0)
		(size 0.4 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy 0.32 -0.125) (xy 0.7 -0.125) (xy 0.7 0.125) (xy 0.32 0.125) (xy 0.2 0.35) (xy -0.2 0.35) (xy -0.32 0.125)
					(xy -0.85 0.125) (xy -0.85 -0.125) (xy -0.32 -0.125) (xy -0.2 -0.35) (xy 0.2 -0.35)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "3" smd roundrect
		(at -0.675 0.5)
		(size 0.35 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at 0.675 0.5)
		(size 0.35 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at 0.675 -0.5)
		(size 0.35 0.25)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/HVSOF5.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
