(footprint "Infineon_PG-HSOF-8-2_ThermalVias"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "HSOF-8-2 [TOLL] power MOSFET (http://www.infineon.com/cms/en/product/packages/PG-HSOF/PG-HSOF-8-2/)")
	(tags "mosfet hsof toll thermal vias")
	(property "Reference" "REF**"
		(at 0 -6 0)
		(layer "F.SilkS")
	)
	(property "Value" "Infineon_PG-HSOF-8-2_ThermalVias"
		(at 0 6 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd rect
		(at -5.4 -4.2)
		(size 2.35 0.7)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -5.4 -3)
		(size 2.35 0.7)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -5.4 -1.8)
		(size 2.35 0.7)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -5.4 -0.6)
		(size 2.35 0.7)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -5.4 0.6)
		(size 2.35 0.7)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -5.4 1.8)
		(size 2.35 0.7)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -5.4 3)
		(size 2.35 0.7)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -5.4 4.2)
		(size 2.35 0.7)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at -0.12 -4.2)
		(size 1 1)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at -0.12 -3)
		(size 1 1)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at -0.12 -1.8)
		(size 1 1)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at -0.12 -0.6)
		(size 1 1)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at -0.12 0.6)
		(size 1 1)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at -0.12 1.8)
		(size 1 1)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at -0.12 3)
		(size 1 1)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at -0.12 4.2)
		(size 1 1)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at 1.08 -4.2)
		(size 1 1)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at 1.08 -3)
		(size 1 1)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at 1.08 -1.8)
		(size 1 1)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at 1.08 -0.6)
		(size 1 1)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at 1.08 0.6)
		(size 1 1)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at 1.08 1.8)
		(size 1 1)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at 1.08 3)
		(size 1 1)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at 1.08 4.2)
		(size 1 1)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at 2.28 -3)
		(size 1 1)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at 2.28 -1.8)
		(size 1 1)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at 2.28 -0.6)
		(size 1 1)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at 2.28 0.6)
		(size 1 1)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at 2.28 1.8)
		(size 1 1)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at 2.28 3)
		(size 1 1)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at 3.48 -3)
		(size 1 1)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at 3.48 -1.8)
		(size 1 1)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at 3.48 -0.6)
		(size 1 1)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at 3.48 0.6)
		(size 1 1)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at 3.48 1.8)
		(size 1 1)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at 3.48 3)
		(size 1 1)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at 4.68 -3)
		(size 1 1)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at 4.68 -1.8)
		(size 1 1)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at 4.68 -0.6)
		(size 1 1)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at 4.68 0.6)
		(size 1 1)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at 4.68 1.8)
		(size 1 1)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at 4.68 3)
		(size 1 1)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at 5.88 -4.2)
		(size 1 1)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at 5.88 -3)
		(size 1 1)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at 5.88 -1.8)
		(size 1 1)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at 5.88 -0.6)
		(size 1 1)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at 5.88 0.6)
		(size 1 1)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at 5.88 1.8)
		(size 1 1)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at 5.88 3)
		(size 1 1)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at 5.88 4.2)
		(size 1 1)
		(layers "F.Paste")
	)
	(pad "1" smd rect
		(at -5.4 -4.2)
		(size 2.5 0.8)
		(layers "F.Cu" "F.Mask")
	)
	(pad "2" smd rect
		(at -5.4 -3)
		(size 2.5 0.8)
		(layers "F.Cu" "F.Mask")
	)
	(pad "3" smd custom
		(at -4.4 1.2)
		(size 0.5 6.8)
		(layers "F.Cu" "F.Mask")
		(zone_connect 2)
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.25 -2.6) (xy -2.25 -2.6) (xy -2.25 -3.4) (xy -0.25 -3.4)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy -0.25 -1.4) (xy -2.25 -1.4) (xy -2.25 -2.2) (xy -0.25 -2.2)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy -0.25 -0.2) (xy -2.25 -0.2) (xy -2.25 -1) (xy -0.25 -1)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy -0.25 1) (xy -2.25 1) (xy -2.25 0.2) (xy -0.25 0.2)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy -0.25 2.2) (xy -2.25 2.2) (xy -2.25 1.4) (xy -0.25 1.4)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy -0.25 3.4) (xy -2.25 3.4) (xy -2.25 2.6) (xy -0.25 2.6)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "4" thru_hole circle
		(at -0.72 -3.6)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at -0.72 -2.4)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at -0.72 -1.2)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at -0.72 0)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at -0.72 1.2)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at -0.72 2.4)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at -0.72 3.6)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 0.48 -3.6)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 0.48 -2.4)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 0.48 -1.2)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 0.48 0)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 0.48 1.2)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 0.48 2.4)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 0.48 3.6)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 1.68 -3.6)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 1.68 -2.4)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 1.68 -1.2)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 1.68 0)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 1.68 1.2)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 1.68 2.4)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 1.68 3.6)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 2.88 -3.6)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 2.88 -2.4)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 2.88 -1.2)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 2.88 0)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 2.88 1.2)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 2.88 2.4)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 2.88 3.6)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "4" smd custom
		(at 3.75 0)
		(size 2.8 8.7)
		(layers "F.Cu" "F.Mask")
		(zone_connect 2)
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy 2.9 5.05) (xy 1.4 5.05) (xy 1.4 -5.05) (xy 2.9 -5.05)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy -1.4 4.85) (xy -5.1 4.85) (xy -5.1 -4.85) (xy -1.4 -4.85)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "4" smd custom
		(at 3.75 0)
		(size 2.8 8.7)
		(layers "B.Cu")
		(zone_connect 2)
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy 2.9 5.05) (xy 1.4 5.05) (xy 1.4 -5.05) (xy 2.9 -5.05)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy -1.4 4.85) (xy -5.1 4.85) (xy -5.1 -4.85) (xy -1.4 -4.85)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "4" thru_hole circle
		(at 4.08 -3.6)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 4.08 -2.4)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 4.08 -1.2)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 4.08 0)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 4.08 1.2)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 4.08 2.4)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 4.08 3.6)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 5.28 -3.6)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 5.28 -2.4)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 5.28 -1.2)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 5.28 0)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 5.28 1.2)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 5.28 2.4)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 5.28 3.6)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/Infineon_PG-HSOF-8-2.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
