(footprint "Infineon_PG-TO-220-7Lead_TabPin8"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Infineon PG-TO-220-7, Tab as Pin 8, see e.g. https://www.infineon.com/dgdl/Infineon-BTS50055-1TMC-DS-v01_00-EN.pdf?fileId=5546d4625a888733015aa9b0007235e9")
	(tags "Infineon PG-TO-220-7")
	(property "Reference" "REF**"
		(at -1.2625 -6.5 0)
		(layer "F.SilkS")
	)
	(property "Value" "Infineon_PG-TO-220-7Lead_TabPin8"
		(at -1.2625 6.5 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 1.3875 -0.1 0)
		(layer "F.Fab")
	)
	(pad "" smd roundrect
		(at -0.2625 -2.75)
		(size 4.6 5.3)
		(layers "F.Paste")
		(roundrect_rratio 0.05434782609)
	)
	(pad "" smd roundrect
		(at -0.2625 2.75)
		(size 4.6 5.3)
		(layers "F.Paste")
		(roundrect_rratio 0.05434782609)
	)
	(pad "" smd roundrect
		(at 4.4875 -2.75)
		(size 4.6 5.3)
		(layers "F.Paste")
		(roundrect_rratio 0.05434782609)
	)
	(pad "" smd roundrect
		(at 4.4875 2.75)
		(size 4.6 5.3)
		(layers "F.Paste")
		(roundrect_rratio 0.05434782609)
	)
	(pad "1" smd roundrect
		(at -7.0375 -3.81)
		(size 4.6 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -7.0375 -2.54)
		(size 4.6 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at -7.0375 -1.27)
		(size 4.6 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at -7.0375 0)
		(size 4.6 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at -7.0375 1.27)
		(size 4.6 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "6" smd roundrect
		(at -7.0375 2.54)
		(size 4.6 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "7" smd roundrect
		(at -7.0375 3.81)
		(size 4.6 0.8)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "8" smd roundrect
		(at 2.1125 0)
		(size 9.4 10.8)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.02659574468)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/Infineon_PG-TO-220-7Lead_TabPin8.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
