(footprint "LFPAK33"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "LFPAK33 SOT-1210 https://assets.nexperia.com/documents/outline-drawing/SOT1210.pdf")
	(tags "LFPAK33 SOT-1210")
	(property "Reference" "REF**"
		(at 0 -2.55 0)
		(layer "F.SilkS")
	)
	(property "Value" "LFPAK33"
		(at 0 2.64 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 90)
		(layer "F.Fab")
	)
	(pad "" smd roundrect
		(at -1.535 -0.975)
		(size 0.83 0.3)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -1.535 -0.325)
		(size 0.83 0.3)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -1.535 0.325)
		(size 0.83 0.3)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -1.535 0.975)
		(size 0.83 0.3)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -0.215 -0.626)
		(size 0.51 0.635)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -0.215 0.626)
		(size 0.51 0.635)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 0.645 -0.626)
		(size 0.51 0.635)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 0.645 0.626)
		(size 0.51 0.635)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 1.575 -0.975)
		(size 0.83 0.3)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 1.575 -0.325)
		(size 0.83 0.3)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 1.575 0.325)
		(size 0.83 0.3)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 1.575 0.975)
		(size 0.83 0.3)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "1" smd roundrect
		(at -1.535 -0.975)
		(size 0.83 0.4)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -1.535 -0.325)
		(size 0.83 0.4)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at -1.535 0.325)
		(size 0.83 0.4)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at -1.535 0.975)
		(size 0.83 0.4)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd custom
		(at 0.405 0)
		(size 1.85 2.25)
		(layers "F.Cu" "F.Mask")
		(zone_connect 2)
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy 1.545 -0.775) (xy 0.925 -0.775) (xy 0.925 -1.175) (xy 1.545 -1.175)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 1.545 -0.125) (xy 0.925 -0.125) (xy 0.925 -0.525) (xy 1.545 -0.525)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 1.545 0.525) (xy 0.925 0.525) (xy 0.925 0.125) (xy 1.545 0.125)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 1.545 1.175) (xy 0.925 1.175) (xy 0.925 0.775) (xy 1.545 0.775)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/LFPAK33.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
