(footprint "LFPAK56"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "LFPAK56 https://assets.nexperia.com/documents/outline-drawing/SOT669.pdf")
	(tags "LFPAK56 SOT-669 Power-SO8")
	(property "Reference" "REF**"
		(at -0.08 -3.48 0)
		(layer "F.SilkS")
	)
	(property "Value" "LFPAK56"
		(at -0.245 3.52 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(solder_paste_margin -0.05)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0.165 0 90)
		(layer "F.Fab")
	)
	(pad "" smd roundrect
		(at -0.5 -1.15)
		(size 0.6 0.9)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -0.5 0)
		(size 0.6 0.9)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -0.5 1.15)
		(size 0.6 0.9)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 0.35 -1.15)
		(size 0.6 0.9)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 0.35 0)
		(size 0.6 0.9)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 0.35 1.15)
		(size 0.6 0.9)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 1.2 -1.15)
		(size 0.6 0.9)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 1.2 0)
		(size 0.6 0.9)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 1.2 1.15)
		(size 0.6 0.9)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 3.05 -1.88 270)
		(size 0.6 0.9)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 3.05 -0.6 270)
		(size 0.6 0.9)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 3.05 0.6 270)
		(size 0.6 0.9)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 3.05 1.88 270)
		(size 0.6 0.9)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "1" smd roundrect
		(at -2.67 -1.91 270)
		(size 0.7 1.15)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -2.67 -0.64 270)
		(size 0.7 1.15)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at -2.67 0.64 270)
		(size 0.7 1.15)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at -2.67 1.91 270)
		(size 0.7 1.15)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd custom
		(at 0.6 0)
		(size 3.3 4.2)
		(layers "F.Cu" "F.Mask")
		(zone_connect 2)
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy 2.975 2.35) (xy 1.425 2.35) (xy 1.425 -2.35) (xy 2.975 -2.35)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/LFPAK56.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
