(footprint "LFPAK88"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "LFPAK88 PowerPAK 8 x 8L BWL Single SOT-1235 (https://assets.nexperia.com/documents/package-information/SOT1235.pdf)")
	(tags "PowerPAK 8x8L Nexperia Vishay")
	(property "Reference" "REF**"
		(at 0 -5.25 0)
		(layer "F.SilkS")
	)
	(property "Value" "LFPAK88"
		(at 0 5.25 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -3.82 -3)
		(size 1.4 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -3.82 -1)
		(size 1.4 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at -3.82 1)
		(size 1.4 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at -3.82 3)
		(size 1.4 1.2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at -0.55 -2.25)
		(size 1.15 2.05)
		(layers "F.Cu" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at -0.55 0)
		(size 1.15 2.05)
		(layers "F.Cu" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at -0.55 2.25)
		(size 1.15 2.05)
		(layers "F.Cu" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd custom
		(at 0.65 0)
		(size 3.74 6.8)
		(layers "F.Cu" "F.Mask")
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy 1.87 3.4) (xy 1.87 4.3) (xy 3.63 4.3) (xy 3.63 -4.3) (xy 1.87 -4.3) (xy 1.87 -3.4)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "5" smd roundrect
		(at 0.8 -2.25)
		(size 1.15 2.05)
		(layers "F.Cu" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at 0.8 0)
		(size 1.15 2.05)
		(layers "F.Cu" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at 0.8 2.25)
		(size 1.15 2.05)
		(layers "F.Cu" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at 2.15 -2.25)
		(size 1.15 2.05)
		(layers "F.Cu" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at 2.15 0)
		(size 1.15 2.05)
		(layers "F.Cu" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at 2.15 2.25)
		(size 1.15 2.05)
		(layers "F.Cu" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at 3.55 -3.55)
		(size 1.25 1.2)
		(layers "F.Cu" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at 3.55 0)
		(size 1.25 0.7)
		(layers "F.Cu" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at 3.55 3.55)
		(size 1.25 1.2)
		(layers "F.Cu" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at 3.825 -1.7)
		(size 0.7 2.1)
		(layers "F.Cu" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at 3.825 1.7)
		(size 0.7 2.1)
		(layers "F.Cu" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/LFPAK88.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
