(footprint "Nexperia_CFP15_SOT-1289"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Nexperia CFP15 (SOT-1289), https://assets.nexperia.com/documents/outline-drawing/SOT1289.pdf")
	(tags "SOT-1289 CFP15")
	(property "Reference" "REF**"
		(at 0 -3 0)
		(layer "F.SilkS")
	)
	(property "Value" "Nexperia_CFP15_SOT-1289"
		(at 0 3 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 -3 0)
		(layer "F.Fab")
	)
	(pad "" smd roundrect
		(at -0.4 -0.95 180)
		(size 1.9 1.7)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -0.4 0.95 180)
		(size 1.9 1.7)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 1.7 -0.95 180)
		(size 1.9 1.7)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 1.7 0.95 180)
		(size 1.9 1.7)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 3.15 0 180)
		(size 0.6 2.4)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "1" smd roundrect
		(at -2.78 -1.065 180)
		(size 1.44 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -2.78 1.065 180)
		(size 1.44 1.6)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd rect
		(at 1.02 0 180)
		(size 4.96 3.8)
		(layers "F.Cu" "F.Mask")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/Nexperia_CFP15_SOT-1289.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
