(footprint "PQFN_8x8"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Low Profile 8x8mm PQFN, Dual Cool 88, https://www.onsemi.com/pub/Collateral/FDMT80080DC-D.pdf")
	(tags "pqfn vdfn mosfet")
	(property "Reference" "REF**"
		(at 0 -4.9 0)
		(layer "F.SilkS")
	)
	(property "Value" "PQFN_8x8"
		(at 0 5 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd roundrect
		(at -0.5 -2.25 270)
		(size 1.5 1.5)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -0.5 0 270)
		(size 1.5 1.5)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -0.5 2.25 270)
		(size 1.5 1.5)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 2 -2.25 270)
		(size 1.5 1.5)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 2 0 270)
		(size 1.5 1.5)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 2 2.25 270)
		(size 1.5 1.5)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "1" smd roundrect
		(at -3.935 -3)
		(size 1.13 1.1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd custom
		(at -3.61 1)
		(size 0.48 5.1)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(zone_connect 2)
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.24 -1.45) (xy -0.89 -1.45) (xy -0.89 -2.55) (xy -0.24 -2.55)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy -0.24 0.55) (xy -0.89 0.55) (xy -0.89 -0.55) (xy -0.24 -0.55)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy -0.24 2.55) (xy -0.89 2.55) (xy -0.89 1.45) (xy -0.24 1.45)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "3" smd custom
		(at 0.785 0)
		(size 5.23 6.9)
		(layers "F.Cu" "F.Mask")
		(zone_connect 2)
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy 3.715 -2.45) (xy 2.615 -2.45) (xy 2.615 -3.55) (xy 3.715 -3.55)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 3.715 -0.45) (xy 2.615 -0.45) (xy 2.615 -1.55) (xy 3.715 -1.55)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 3.715 1.55) (xy 2.615 1.55) (xy 2.615 0.45) (xy 3.715 0.45)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 3.715 3.55) (xy 2.615 3.55) (xy 2.615 2.45) (xy 3.715 2.45)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/PQFN_8x8.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
