(footprint "ROHM_SOT-457_ClockwisePinNumbering"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "ROHM SOT-457 SC-74, 6 Pin (https://fscdn.rohm.com/en/products/databook/datasheet/discrete/transistor/digital/imh3at110-e.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
	(tags "ROHM SC-74 TO_SOT_SMD")
	(property "Reference" "REF**"
		(at 0 -2.8 0)
		(layer "F.SilkS")
	)
	(property "Value" "ROHM_SOT-457_ClockwisePinNumbering"
		(at 0 2.8 0)
		(layer "F.Fab")
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -0.95 -1.1)
		(size 0.5 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at 0 -1.1)
		(size 0.5 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at 0.95 -1.1)
		(size 0.5 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at 0.95 1.1)
		(size 0.5 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at 0 1.1)
		(size 0.5 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "6" smd roundrect
		(at -0.95 1.1)
		(size 0.5 1.5)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/ROHM_SOT-457_ClockwisePinNumbering.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
