(footprint "Rohm_HRP7"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Rohm HRP7 SMD package, http://rohmfs.rohm.com/en/techdata_basic/ic/package/hrp7_1-e.pdf, http://rohmfs.rohm.com/en/products/databook/datasheet/ic/motor/dc/bd621x-e.pdf")
	(tags "Rohm HRP7 SMD")
	(property "Reference" "REF**"
		(at -0.015 -5.9 0)
		(layer "F.SilkS")
	)
	(property "Value" "Rohm_HRP7"
		(at -0.015 6 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at -0.015 0 0)
		(layer "F.Fab")
	)
	(pad "" smd roundrect
		(at -1.11 -2.5)
		(size 4 4.5)
		(layers "F.Paste")
		(roundrect_rratio 0.0625)
	)
	(pad "" smd roundrect
		(at -1.11 2.5)
		(size 4 4.5)
		(layers "F.Paste")
		(roundrect_rratio 0.0625)
	)
	(pad "" smd roundrect
		(at 3.39 -2.5)
		(size 4 4.5)
		(layers "F.Paste")
		(roundrect_rratio 0.0625)
	)
	(pad "" smd roundrect
		(at 3.39 2.5)
		(size 4 4.5)
		(layers "F.Paste")
		(roundrect_rratio 0.0625)
	)
	(pad "1" smd roundrect
		(at -4.985 -3.81)
		(size 1.37 0.93)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -4.985 -2.54)
		(size 1.37 0.93)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at -4.985 -1.27)
		(size 1.37 0.93)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at -4.985 0)
		(size 1.37 0.93)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "4" thru_hole circle
		(at -2.46 -4.2)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at -2.46 -3)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at -2.46 -1.8)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at -2.46 -0.6)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at -2.46 0.6)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at -2.46 1.8)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at -2.46 3)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at -2.46 4.2)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at -1.26 -4.2)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at -1.26 -3)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at -1.26 -1.8)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at -1.26 -0.6)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at -1.26 0.6)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at -1.26 1.8)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at -1.26 3)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at -1.26 4.2)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at -0.06 -4.2)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at -0.06 -3)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at -0.06 -1.8)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at -0.06 -0.6)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at -0.06 0.6)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at -0.06 1.8)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at -0.06 3)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at -0.06 4.2)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 1.14 -4.2)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 1.14 -3)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 1.14 -1.8)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 1.14 -0.6)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "4" smd roundrect
		(at 1.14 0)
		(size 9 10)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.02777777778)
	)
	(pad "4" smd roundrect
		(at 1.14 0)
		(size 9 10)
		(layers "B.Cu")
		(roundrect_rratio 0.02777777778)
	)
	(pad "4" thru_hole circle
		(at 1.14 0.6)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 1.14 1.8)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 1.14 3)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 1.14 4.2)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 2.34 -4.2)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 2.34 -3)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 2.34 -1.8)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 2.34 -0.6)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 2.34 0.6)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 2.34 1.8)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 2.34 3)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 2.34 4.2)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 3.54 -4.2)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 3.54 -3)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 3.54 -1.8)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 3.54 -0.6)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 3.54 0.6)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 3.54 1.8)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 3.54 3)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 3.54 4.2)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 4.74 -4.2)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 4.74 -3)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 4.74 -1.8)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 4.74 -0.6)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 4.74 0.6)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 4.74 1.8)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 4.74 3)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole circle
		(at 4.74 4.2)
		(size 0.6 0.6)
		(drill 0.3)
		(layers "*.Cu")
		(remove_unused_layers no)
	)
	(pad "5" smd roundrect
		(at -4.985 1.27)
		(size 1.37 0.93)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "6" smd roundrect
		(at -4.985 2.54)
		(size 1.37 0.93)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "7" smd roundrect
		(at -4.985 3.81)
		(size 1.37 0.93)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/Rohm_HRP7.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
