(footprint "SOT-553"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "SOT, 5 Pin (https://www.jedec.org/system/files/docs/MO-293B.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
	(tags "SOT TO_SOT_SMD JEDEC-MO-293-UAAD-1 Texas-DRL-5")
	(property "Reference" "REF**"
		(at 0 -1.65 0)
		(layer "F.SilkS")
	)
	(property "Value" "SOT-553"
		(at 0 1.65 0)
		(layer "F.Fab")
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -0.7125 -0.5)
		(size 0.675 0.35)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "2" smd roundrect
		(at -0.7125 0)
		(size 0.675 0.35)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "3" smd roundrect
		(at -0.7125 0.5)
		(size 0.675 0.35)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "4" smd roundrect
		(at 0.7125 0.5)
		(size 0.675 0.35)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(pad "5" smd roundrect
		(at 0.7125 -0.5)
		(size 0.675 0.35)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.25)
	)
	(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-553.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
