(footprint "TDSON-8-1"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "Power MOSFET package, TDSON-8-1, 5.15x5.9mm (https://www.infineon.com/cms/en/product/packages/PG-TDSON/PG-TDSON-8-1/)")
	(tags "tdson ")
	(property "Reference" "REF**"
		(at 0 -3.5 0)
		(layer "F.SilkS")
	)
	(property "Value" "TDSON-8-1"
		(at 0 3.5 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd roundrect
		(at -0.2 -0.85)
		(size 1.5 1.5)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at -0.2 0.85)
		(size 1.5 1.5)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd custom
		(at 0.65 0)
		(size 3.75 4.41)
		(layers "F.Mask")
		(zone_connect 0)
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy 2.675 -1.605) (xy 1.875 -1.605) (xy 1.875 -2.205) (xy 2.675 -2.205)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 2.675 -0.335) (xy 1.875 -0.335) (xy 1.875 -0.935) (xy 2.675 -0.935)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 2.675 0.935) (xy 1.875 0.935) (xy 1.875 0.335) (xy 2.675 0.335)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy 2.675 2.205) (xy 1.875 2.205) (xy 1.875 1.605) (xy 2.675 1.605)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "" smd roundrect
		(at 1.5 -0.85)
		(size 1.5 1.5)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 1.5 0.85)
		(size 1.5 1.5)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 2.905 -1.905)
		(size 0.75 0.5)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 2.905 -0.635)
		(size 0.75 0.5)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 2.905 0.635)
		(size 0.75 0.5)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "" smd roundrect
		(at 2.905 1.905)
		(size 0.75 0.5)
		(layers "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "1" smd roundrect
		(at -2.9 -1.905)
		(size 0.85 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_paste_margin -0.05)
	)
	(pad "2" smd roundrect
		(at -2.9 -0.635)
		(size 0.85 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_paste_margin -0.05)
	)
	(pad "3" smd roundrect
		(at -2.9 0.635)
		(size 0.85 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_paste_margin -0.05)
	)
	(pad "4" smd roundrect
		(at -2.9 1.905)
		(size 0.85 0.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
		(solder_paste_margin -0.05)
	)
	(pad "5" smd rect
		(at 1.05 0)
		(size 4.55 4.41)
		(layers "F.Cu")
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/TDSON-8-1.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
