(footprint "TO-252-2_TabPin1"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "TO-252-2, tab to pin 1 https://www.wolfspeed.com/media/downloads/87/CSD01060.pdf")
	(tags "TO-252-2 diode")
	(property "Reference" "REF**"
		(at -1.375 -4.55 0)
		(layer "F.SilkS")
	)
	(property "Value" "TO-252-2_TabPin1"
		(at -1.425 4.8 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at -0.85 0 0)
		(layer "F.Fab")
	)
	(pad "" smd roundrect
		(at 0.25 -1.8 270)
		(size 3.3 3.3)
		(layers "F.Paste")
		(roundrect_rratio 0.07575757576)
	)
	(pad "" smd roundrect
		(at 0.25 1.8 270)
		(size 3.3 3.3)
		(layers "F.Paste")
		(roundrect_rratio 0.07575757576)
	)
	(pad "" smd roundrect
		(at 3.8 -1.8 270)
		(size 3.3 3.3)
		(layers "F.Paste")
		(roundrect_rratio 0.07575757576)
	)
	(pad "" smd roundrect
		(at 3.8 1.8 270)
		(size 3.3 3.3)
		(layers "F.Paste")
		(roundrect_rratio 0.07575757576)
	)
	(pad "1" smd roundrect
		(at -5.375 -2.3)
		(size 3.5 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(pad "1" smd roundrect
		(at 2.025 0)
		(size 7 7)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.03571428571)
	)
	(pad "2" smd roundrect
		(at -5.375 2.28)
		(size 3.5 2)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.25)
	)
	(embedded_fonts no)
	(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/TO-252-2.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
