(footprint "TO-252-3_TabPin2"
	(version 20240108)
	(generator "kicad-footprint-generator")
	(layer "F.Cu")
	(descr "TO-252/DPAK SMD package, http://www.infineon.com/cms/en/product/packages/PG-TO252/PG-TO252-3-1/")
	(tags "DPAK TO-252 DPAK-3 TO-252-3 SOT-428")
	(property "Reference" "REF**"
		(at 0 -4.5 0)
		(layer "F.SilkS")
	)
	(property "Value" "TO-252-3_TabPin2"
		(at 0 4.5 0)
		(layer "F.Fab")
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd roundrect
		(at -5.04 -2.28)
		(size 2.2 1.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.208333)
	)
	(pad "2" smd roundrect
		(at -5.04 0)
		(size 2.2 1.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.208333)
	)
	(pad "2" smd roundrect
		(at -0.415 -1.525)
		(size 3.05 2.75)
		(layers "F.Cu" "F.Paste")
		(roundrect_rratio 0.090909)
	)
	(pad "2" smd roundrect
		(at -0.415 1.525)
		(size 3.05 2.75)
		(layers "F.Cu" "F.Paste")
		(roundrect_rratio 0.090909)
	)
	(pad "2" smd roundrect
		(at 1.26 0)
		(size 6.4 5.8)
		(layers "F.Cu" "F.Mask")
		(roundrect_rratio 0.043103)
	)
	(pad "2" smd roundrect
		(at 2.935 -1.525)
		(size 3.05 2.75)
		(layers "F.Cu" "F.Paste")
		(roundrect_rratio 0.090909)
	)
	(pad "2" smd roundrect
		(at 2.935 1.525)
		(size 3.05 2.75)
		(layers "F.Cu" "F.Paste")
		(roundrect_rratio 0.090909)
	)
	(pad "3" smd roundrect
		(at -5.04 2.28)
		(size 2.2 1.2)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(roundrect_rratio 0.208333)
	)
	(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/TO-252-3_TabPin2.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
